Macros
State from Software CS De-Assert
Peripheral Driver » HAL Driver » SPI » Defines
Collaboration diagram for State from Software CS De-Assert:

## Macros
#define | CS_END_STATE_POLL_TX 0x81
| State from Software CS De-Assert. More...
#define | CS_END_STATE_POLL_RX 0x82
| CS DE-ASSERT when Receiving Ends by Polling. More...
#define | CS_END_STATE_POLL_TX_RX 0x83
| CS DE-ASSERT when DUPLEX Ends by Polling. More...
#define | CS_END_STATE_POLL_EEPREAD 0x84
| CS DE-ASSERT when EEPREAD Ends by Polling. More...
#define | CS_END_STATE_TX_CPLT 0x90
| CS DE-ASSERT when Transferring Ends by IT/DMA. More...
#define | CS_END_STATE_RX_CPLT 0x91
| CS DE-ASSERT when Receiving Ends by IT/DMA. More...
#define | CS_END_STATE_TX_RX_CPLT 0x92
| CS DE-ASSERT when DUPLEX Ends by IT/DMA. More...
#define | CS_END_STATE_XFER_ERR 0x93
| CS DE-ASSERT when xfer Error by IT/DMA. More...
#define | CS_END_STATE_TX_ABORT_CPLT 0x94
| CS DE-ASSERT when abort The transfer Ends by IT/DMA. More...
#define | CS_END_STATE_RX_ABORT_CPLT 0x95
| CS DE-ASSERT when abort the receive Ends by IT/DMA. More...
#define | CS_END_STATE_ABORT_CPLT 0x96
| CS DE-ASSERT when abort the tx/rx by IT/DMA. More...

## Detailed Description

## Macro Definition Documentation

## ◆ CS_END_STATE_ABORT_CPLT

#define CS_END_STATE_ABORT_CPLT 0x96

CS DE-ASSERT when abort the tx/rx by IT/DMA.

Definition at line 181 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_POLL_EEPREAD

#define CS_END_STATE_POLL_EEPREAD 0x84

CS DE-ASSERT when EEPREAD Ends by Polling.

Definition at line 174 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_POLL_RX

#define CS_END_STATE_POLL_RX 0x82

CS DE-ASSERT when Receiving Ends by Polling.

Definition at line 172 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_POLL_TX

#define CS_END_STATE_POLL_TX 0x81

State from Software CS De-Assert.

CS DE-ASSERT when Transferring Ends by Polling

Definition at line 171 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_POLL_TX_RX

#define CS_END_STATE_POLL_TX_RX 0x83

CS DE-ASSERT when DUPLEX Ends by Polling.

Definition at line 173 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_RX_ABORT_CPLT

#define CS_END_STATE_RX_ABORT_CPLT 0x95

CS DE-ASSERT when abort the receive Ends by IT/DMA.

Definition at line 180 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_RX_CPLT

#define CS_END_STATE_RX_CPLT 0x91

CS DE-ASSERT when Receiving Ends by IT/DMA.

Definition at line 176 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_TX_ABORT_CPLT

#define CS_END_STATE_TX_ABORT_CPLT 0x94

CS DE-ASSERT when abort The transfer Ends by IT/DMA.

Definition at line 179 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_TX_CPLT

#define CS_END_STATE_TX_CPLT 0x90

CS DE-ASSERT when Transferring Ends by IT/DMA.

Definition at line 175 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_TX_RX_CPLT

#define CS_END_STATE_TX_RX_CPLT 0x92

CS DE-ASSERT when DUPLEX Ends by IT/DMA.

Definition at line 177 of file gr55xx_hal_spi.h.

## ◆ CS_END_STATE_XFER_ERR

#define CS_END_STATE_XFER_ERR 0x93

CS DE-ASSERT when xfer Error by IT/DMA.

Definition at line 178 of file gr55xx_hal_spi.h.