Modules
QSPI Exported Constants
Peripheral Driver » LL Driver » QSPI » Defines
Collaboration diagram for QSPI Exported Constants:

## Modules
| FIFO Depth Defines
| Get Flags Defines
| Flags definitions which can be used with LL_QSPI_ReadReg function.
| IT Defines
| Interrupt definitions which can be used with LL_QSPI_ReadReg and LL_QSPI_WriteReg functions.
| SPI Frame Format
| Datawidth
| MicroWire CommandSize
| Test Mode
| Slave Out Enable
| Transfer Mode
| Clock Phase
| Clock Polarity
| Serial Protocol
| MicroWire Control
| Slave Select
| DMA Defines
| QSPI Instruction Size
| QSPI Address Size
| QSPI RX SAMPLE EDGE
| QSPI Address and Instruction Transfer Format
| Endian mode For XIP
| Endian mode for qspi xip.
| Slave For XIP
| Which Slave to Enable in XIP.
| Data Frame Size For Xip
| Data frame size in xip, take effect when enable DFS_HC.
| Mode Bits Length For Xip
| Instruction Size For Xip
| Address Size For Xip
| Address size for concurrent xip mode.
| Instruction And Address For Xip
| Transfer of inst & address for concurrent xip mode.
| Frame Format For Xip
| Frame format for concurrent xip mode.
| Mode Clock stretch mode
| Prefetch Defines
| CONT XFERR Defines
| Instruction Defines
| Mode Bits Defines
| DFS Hardcode Defines
| Instruction Sent Mode
| InitStrcut default configuartion

## Detailed Description