Macros
AON_GPIO Exported Macros
Peripheral Driver » HAL Driver » AON_GPIO » Defines
Collaboration diagram for AON_GPIO Exported Macros:

## Macros
#define | __HAL_AON_GPIO_IT_GET_IT(__AON_GPIO_PIN__) ll_aon_gpio_read_flag_it(__AON_GPIO_PIN__)
| Check whether the specified AON_GPIO pin is asserted or not. More...
#define | __HAL_AON_GPIO_IT_CLEAR_IT(__AON_GPIO_PIN__) ll_aon_gpio_clear_flag_it(__AON_GPIO_PIN__)
| Clear the AON_GPIO pin pending bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ __HAL_AON_GPIO_IT_CLEAR_IT

#define __HAL_AON_GPIO_IT_CLEAR_IT | ( |  | __AON_GPIO_PIN__ | ) | ll_aon_gpio_clear_flag_it(__AON_GPIO_PIN__)

Clear the AON_GPIO pin pending bits.

Parameters

  <strong>AON_GPIO_PIN</strong> | specifies the AON_GPIO pins to be cleared. This parameter can be any combination of AON_GPIO_PIN_x where x can be (0..7).

Return values

  None |

Definition at line 208 of file gr55xx_hal_aon_gpio.h.

## ◆ __HAL_AON_GPIO_IT_GET_IT

#define __HAL_AON_GPIO_IT_GET_IT | ( |  | __AON_GPIO_PIN__ | ) | ll_aon_gpio_read_flag_it(__AON_GPIO_PIN__)

Check whether the specified AON_GPIO pin is asserted or not.

Parameters

  <strong>AON_GPIO_PIN</strong> | specifies the AON_GPIO pin to be checked. This parameter can be AON_GPIO_PIN_x where x can be (0..7).

Return values

  The | new state of AON_GPIO_PIN (SET or RESET).

Definition at line 200 of file gr55xx_hal_aon_gpio.h.