### - r -

- ras_ad_init() : ras_ad.h
- ras_ad_send_noti_ind() : ras_ad.h
- ras_c_ad_disconnect_handler() : ras_c_ad.h
- ras_c_ad_init() : ras_c_ad.h
- ras_c_ad_read_char() : ras_c_ad.h
- ras_c_ad_start_discov_srvc() : ras_c_ad.h
- ras_c_ad_write_char() : ras_c_ad.h
- ras_c_char_cccd_set() : ras_c.h
- ras_c_connect_handler() : ras_c.h
- ras_c_disconnect_handler() : ras_c.h
- ras_c_discov_srvc_start() : ras_c.h
- ras_c_filter_policy_set() : ras_c.h
- ras_c_free_subevt_data_buff() : ras_c.h
- ras_c_init() : ras_c.h
- ras_c_mtu_exch_handler() : ras_c.h
- ras_c_operation_abort() : ras_c.h
- ras_c_set_remote_step_data_len() : ras_c.h
- ras_connect_handler() : ras.h
- ras_disconnect_handler() : ras.h
- ras_mtu_exch_handler() : ras.h
- ras_proc_disabled_handler() : ras.h
- ras_rcv_subevt_data_handler() : ras.h
- ras_service_init() : ras.h
- ras_set_cache_data_info() : ras.h
- ras_write_subevt_data_free() : ras.h
- restore_sys_context() : gr55xx_sys_sdk.h
- rscs_c_ctrl_pt_indicate_set() : rscs_c.h
- rscs_c_ctrl_pt_set() : rscs_c.h
- rscs_c_disc_srvc_start() : rscs_c.h
- rscs_c_rsc_feature_read() : rscs_c.h
- rscs_c_rsc_meas_notify_set() : rscs_c.h
- rscs_c_sensor_loc_read() : rscs_c.h
- rscs_client_init() : rscs_c.h
- rscs_ctrl_pt_rsp_send() : rscs.h
- rscs_measurement_send() : rscs.h
- rscs_sensor_loc_update() : rscs.h
- rscs_service_init() : rscs.h
- rtus_current_state_set() : rtus.h
- rtus_service_init() : rtus.h
- rtus_update_result_set() : rtus.h