Macros | Functions
gr55xx_ll_cgc.h File Reference

Header file containing functions prototypes of CGC LL library. More...

`#include "gr55xx.h"`
Include dependency graph for gr55xx_ll_cgc.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | LL_CGC_WFI_SECU_HCLK MCU_SUB_WFI_SECU_HCLK
| Hclk for all security blocks More...
#define | LL_CGC_WFI_SIM_HCLK MCU_SUB_WFI_SIM_HCLK
| Hclk for sim card interface More...
#define | LL_CGC_WFI_HTB_HCLK MCU_SUB_WFI_HTB_HCLK
| Hclk for hopping table More...
#define | LL_CGC_WFI_PWM_HCLK MCU_SUB_WFI_PWM_HCLK
| Hclk for PWM More...
#define | LL_CGC_WFI_ROM_HCLK MCU_SUB_WFI_ROM_HCLK
| Hclk for ROM More...
#define | LL_CGC_WFI_SNSADC_HCLK MCU_SUB_WFI_SNSADC_HCLK
| Hclk for sense ADC More...
#define | LL_CGC_WFI_GPIO_HCLK MCU_SUB_WFI_GPIO_HCLK
| Hclk for GPIOs More...
#define | LL_CGC_WFI_BLE_BRG_HCLK MCU_SUB_WFI_BLE_BRG_HCLK
| Hclk for BLE MCU bridge More...
#define | LL_CGC_WFI_APB_SUB_HCLK MCU_SUB_WFI_APB_SUB_HCLK
| Hclk for APB subsystem More...
#define | LL_CGC_WFI_SERIAL_HCLK MCU_SUB_WFI_SERIAL_HCLK
| Hclk for serial blocks More...
#define | LL_CGC_WFI_ALL_HCLK0 ((uint32_t)0x000007FFU)
| All clock group 0 More...
#define | LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK
| Hclk for Always-on register More...
#define | LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK
| Hclk for cache top More...
#define | LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK
| Hclk for SRAMs More...
#define | LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)
| All clock group 1 More...
#define | LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK
| Div4 clk for security blocks More...
#define | LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK
| Div4 clk for xf qspi More...
#define | LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)
| All clock group 2 More...
#define | LL_CGC_FRC_SECU_HCLK MCU_SUB_FORCE_SECU_HCLK
| Hclk for all security blocks More...
#define | LL_CGC_FRC_SIM_HCLK MCU_SUB_FORCE_SIM_HCLK
| Hclk for sim card interface More...
#define | LL_CGC_FRC_HTB_HCLK MCU_SUB_FORCE_HTB_HCLK
| Hclk for hopping table More...
#define | LL_CGC_FRC_ROM_HCLK MCU_SUB_FORCE_ROM_HCLK
| Hclk for ROM More...
#define | LL_CGC_FRC_SNSADC_HCLK MCU_SUB_FORCE_SNSADC_HCLK
| Hclk for sense ADC More...
#define | LL_CGC_FRC_GPIO_HCLK MCU_SUB_FORCE_GPIO_HCLK
| Hclk for GPIOs More...
#define | LL_CGC_FRC_BLE_BRG_HCLK MCU_SUB_FORCE_BLE_BRG_HCLK
| Hclk for BLE MCU bridge More...
#define | LL_CGC_FRC_APB_SUB_HCLK MCU_SUB_FORCE_APB_SUB_HCLK
| Hclk for APB subsystem More...
#define | LL_CGC_FRC_SERIAL_HCLK MCU_SUB_FORCE_SERIAL_HCLK
| Hclk for serial blocks More...
#define | LL_CGC_FRC_USB_HCLK MCU_SUB_FORCE_USB_HCLK
| Hclk for USB More...
#define | LL_CGC_FRC_ALL_HCLK0 ((uint32_t)0x0000177FU)
| All clock group 0 More...
#define | LL_CGC_FRC_AON_MCUSUB_HCLK MCU_SUB_FORCE_AON_MCUSUB_HCLK
| Hclk for Always-on register More...
#define | LL_CGC_FRC_XF_XQSPI_HCLK MCU_SUB_FORCE_XF_XQSPI_HCLK
| Hclk for cache top More...
#define | LL_CGC_FRC_SRAM_HCLK MCU_SUB_FORCE_SRAM_HCLK
| Hclk for SRAMs More...
#define | LL_CGC_FRC_ALL_HCLK1 ((uint32_t)0x00070000U)
| All clock group 1 More...
#define | LL_CGC_FRC_UART0_PCLK MCU_SUB_FORCE_UART0_PCLK
| Pclk for uart0 More...
#define | LL_CGC_FRC_UART1_PCLK MCU_SUB_FORCE_UART1_PCLK
| Pclk for uart1 More...
#define | LL_CGC_FRC_UART2_PCLK MCU_SUB_FORCE_UART2_PCLK
| Pclk for uart2 More...
#define | LL_CGC_FRC_UART3_PCLK MCU_SUB_FORCE_UART3_PCLK
| Pclk for uart3 More...
#define | LL_CGC_FRC_UART4_PCLK MCU_SUB_FORCE_UART4_PCLK
| Pclk for uart4 More...
#define | LL_CGC_FRC_UART5_PCLK MCU_SUB_FORCE_UART5_PCLK
| Pclk for uart5 More...
#define | LL_CGC_FRC_I2C0_PCLK MCU_SUB_FORCE_I2C0_PCLK
| Hclk for i2c0 More...
#define | LL_CGC_FRC_I2C1_PCLK MCU_SUB_FORCE_I2C1_PCLK
| Hclk for i2c1 More...
#define | LL_CGC_FRC_I2C2_PCLK MCU_SUB_FORCE_I2C2_PCLK
| Hclk for i2c2 More...
#define | LL_CGC_FRC_I2C3_PCLK MCU_SUB_FORCE_I2C3_PCLK
| Hclk for i2c3 More...
#define | LL_CGC_FRC_I2C4_PCLK MCU_SUB_FORCE_I2C4_PCLK
| Hclk for i2c4 More...
#define | LL_CGC_FRC_I2C5_PCLK MCU_SUB_FORCE_I2C5_PCLK
| Hclk for i2c5 More...
#define | LL_CGC_FRC_QSPI0_PCLK MCU_SUB_FORCE_QSPI0_PCLK
| Hclk for qspi0 More...
#define | LL_CGC_FRC_QSPI1_PCLK MCU_SUB_FORCE_QSPI1_PCLK
| Hclk for qspi1 More...
#define | LL_CGC_FRC_QSPI2_PCLK MCU_SUB_FORCE_QSPI2_PCLK
| Hclk for qspi2 More...
#define | LL_CGC_FRC_SPI_M_PCLK MCU_SUB_FORCE_SPI_M_PCLK
| Hclk for spim More...
#define | LL_CGC_FRC_SPI_S_PCLK MCU_SUB_FORCE_SPI_S_PCLK
| Hclk for spis More...
#define | LL_CGC_FRC_I2S_HCLK MCU_SUB_FORCE_I2S_PCLK
| Hclk for i2s More...
#define | LL_CGC_FRC_I2S_S_PCLK MCU_SUB_FORCE_I2S_S_PCLK
| Hclk for i2ss More...
#define | LL_CGC_FRC_DSPI_PCLK MCU_SUB_FORCE_DSPI_PCLK
| Hclk for dspi More...
#define | LL_CGC_FRC_PDM_PCLK MCU_SUB_FORCE_PDM_PCLK
| Hclk for pdm More...
#define | LL_CGC_FRC_PWM_0_PCLK MCU_SUB_FORCE_PWM_0_PCLK
| Pclk for PWM0 More...
#define | LL_CGC_FRC_PWM_1_PCLK MCU_SUB_FORCE_PWM_1_PCLK
| Pclk for PWM1 More...
#define | LL_CGC_FRC_VTTBL_PCLK MCU_SUB_FORCE_VTTBL_PCLK
| Pclk for VTTBL More...
#define | LL_CGC_FRC_SECU_DIV4_PCLK MCU_SUB_FORCE_SECU_DIV4_PCLK
| Div4 clk for security blocksi More...
#define | LL_CGC_FRC_XQSPI_DIV4_PCLK MCU_SUB_FORCE_XQSPI_DIV4_PCLK
| Div4 clk for xf qspi More...
#define | LL_CGC_FRC_SERIALS_HCLK2 ((uint32_t)0x705E0FFFUL)
| Hclk for serial blocks More...
#define | LL_CGC_FRC_ALL_HCLK2 ((uint32_t)0xFF7FCFFFUL)
| All clock group 2 More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_ASYNC_EN
| Enable AHB2APB ASYNC low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_SYNC_EN
| Enable AHB2APB SYNC low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_EN MCU_SUB_PERIPH_CG_LP_EN_QSPIM_EN
| Enable qspim low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN MCU_SUB_PERIPH_CG_LP_EN_AHB_BUS_LP_EN
| Enable AHB bus low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN
| Enable i2c sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN
| Enable spis sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN
| Enable spim sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_LP_EN MCU_SUB_PERIPH_CG_LP_EN_I2S_LP_EN
| Enable i2s master low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_PCLK_EN
| Enable uart pclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_SCLK_EN
| Enable uart sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000F3FUL)
| All Low Power Feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0
| Turn the uart0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1
| Turn the uart1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART2
| Turn the uart2 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART3
| Turn the uart3 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART4
| Turn the uart4 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART5
| Turn the uart5 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SM
| Turn the i2s_m off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SS
| Turn the i2s_s off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM
| Turn the spi_m off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS
| Turn the spi_s off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0
| Turn the pwm0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1
| Turn the pwm1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM0
| Turn the qspim0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM1
| Turn the qspim1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM2
| Turn the qspim2 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_DSPI
| Turn the dspi off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PDM
| Turn the pdm off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C2
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C3
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C4
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C5
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x01FC3FFFUL)
| Serial blocks More...
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x03FFFF3FUL)
| Serial blocks More...
#define | LL_CGC_MCU_FRC_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_FORCE_OFF
| Force individual aes's clock control More...
#define | LL_CGC_MCU_SLP_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_SLP_OFF
| Individual aes's clock control More...
#define | LL_CGC_MCU_FRC_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_FORCE_OFF
| Force individual hmac's clock control More...
#define | LL_CGC_MCU_SLP_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_SLP_OFF
| Individual hmac's clock control More...
#define | LL_CGC_MCU_FRC_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_FORCE_OFF
| Force individual pkc's clock control More...
#define | LL_CGC_MCU_SLP_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_SLP_OFF
| Individual pkc's clock control More...
#define | LL_CGC_MCU_FRC_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_FORCE_OFF
| Force individual present's clock control More...
#define | LL_CGC_MCU_SLP_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_SLP_OFF
| Individual present's clock control More...
#define | LL_CGC_MCU_FRC_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_FORCE_OFF
| Force individual ramkey's clock control More...
#define | LL_CGC_MCU_SLP_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_SLP_OFF
| Individual ramkey's clock control More...
#define | LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF
| Force individual rng's clock control More...
#define | LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF
| Individual rng's clock control More...
#define | LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF
| Force individual efuse's clock control More...
#define | LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF
| Individual efuse's clock control More...
#define | LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001555U)
| Hclk for security clock More...
#define | LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002AAAU)
| Hclk for security clock WFI/WFE More...
#define | LL_CGC_MCU_SECU_FRC_OFF_ALL
| Hclk for security clock More...
#define | LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x0000003BU)
| Hclk for msic default clock More...
#define | LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000003FU)
| Hclk for msic all clock More...
#define | LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000038U)
| Hclk for msic dma clock More...
#define | LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK0
| Hclk0 for the system default clock WFI/WFE. More...
#define | LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK1
| Hclk1 for the system default clock WFI/WFE. More...
#define | LL_CGC_MCU_SUBSYS_DEFAULT_CLK
| Hclk for the system default clock More...
#define | LL_CGC_MCU_SUBSYS_DEFAULT_CLK1 (MCU_SUB_FORCE_SECU_DIV4_PCLK)
| Hclk for the system default clock More...
#define | LL_CGC_MCU_PERIPH_CG_DEFAULT
| pclk for the system default periph clock More...
#define | LL_CGC_MCU_PERIPH_SLP_CG_DEFAULT
| pclk for the system default periph wfi clock More...
#define | CGC_CLOCK_ENABLE (1)
| Bit segment address enable More...
#define | CGC_CLOCK_DISABLE (0)
| Bit segment address disable More...
#define | BIT_BAND(addr, bitnum) (((addr) & 0xF0000000) + 0x2000000 + (((addr) & 0xFFFFF) << 5) + ((bitnum) << 2))
| Bit segment address calculation More...
#define | MEMORY_ADDR(addr) (*((volatile uint32_t *)(addr)))
| Bit segment address type conversion More...
#define | BIT_SEGMENT_VALUE(addr, bitnum) MEMORY_ADDR(BIT_BAND(addr, bitnum))
| Bit segment address value manipulation More...

## Functions
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_0 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_0 (void)
| Return to clock blocks that is turned off during WFI. More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_1 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_1 (void)
| Return to clock blocks that is turned off during WFI. More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_2 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_2 (void)
| Return to clock blocks that is turned off during WFI. More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_3 (void)
| Return to clock blocks that is turned off during WFI. More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_4 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_4 (void)
| Return to clock blocks that is turned off during WFI. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_0 (uint32_t clk_mask)
| Some peripherals force turn off clock. More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_0 (void)
| Return to clock blocks that was forcibly closed. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_1 (uint32_t clk_mask)
| Some peripherals force turn off clock. More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_1 (void)
| Return to clock blocks that was forcibly closed. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_2 (uint32_t clk_mask)
| Some peripherals force turn off clock. More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_2 (void)
| Return to clock blocks that was forcibly closed. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock. More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_3 (void)
| Return to clock blocks that is turned off. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_hclk (void)
| Enable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_hclk (void)
| Disable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_hclk (void)
| Indicate whether the security blocks(including AES, PKC, Present, HMAC) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sim_hclk (void)
| Enable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sim_hclk (void)
| Disable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sim_hclk (void)
| Indicate whether the SIM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_htb_hclk (void)
| Enable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_htb_hclk (void)
| Disable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_htb_hclk (void)
| Indicate whether the Hopping Table automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pwm_hclk (void)
| Enable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pwm_hclk (void)
| Disable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pwm_hclk (void)
| Indicate whether the PWM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rom_hclk (void)
| Enable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rom_hclk (void)
| Disable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rom_hclk (void)
| Indicate whether the ROM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_snsadc_hclk (void)
| Enable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_snsadc_hclk (void)
| Disable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_snsadc_hclk (void)
| Indicate whether the SNSADC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_gpio_hclk (void)
| Enable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_gpio_hclk (void)
| Disable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_gpio_hclk (void)
| Indicate whether the GPIO automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_dma_hclk (void)
| Enable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_dma_hclk (void)
| Disable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_dma_hclk (void)
| Indicate whether the DMA automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ble_brg_hclk (void)
| Enable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ble_brg_hclk (void)
| Disable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ble_brg_hclk (void)
| Indicate whether the BLE Bridge automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_apb_sub_hclk (void)
| Enable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_apb_sub_hclk (void)
| Disable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_apb_sub_hclk (void)
| Indicate whether the APB Subsystem automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_serial_hclk (void)
| Enable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_serial_hclk (void)
| Disable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_serial_hclk (void)
| Indicate whether the serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_usb_hclk (void)
| Enable USB automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_usb_hclk (void)
| Disable USB automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_usb_hclk (void)
| Indicate whether the USB automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aon_mcusub_hclk (void)
| Enable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aon_mcusub_hclk (void)
| Disable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk (void)
| Indicate whether the AON_MUCSUB automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_hclk (void)
| Enable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_hclk (void)
| Disable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_hclk (void)
| Indicate whether the XQSPI automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sram_hclk (void)
| Enable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sram_hclk (void)
| Disable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sram_hclk (void)
| Indicate whether the SRAM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_div4_hclk (void)
| Enable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_div4_hclk (void)
| Disable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_div4_hclk (void)
| Indicate whether the security blocks automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_div4_hclk (void)
| Enable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_div4_hclk (void)
| Disable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk (void)
| Indicate whether the XQSPI automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_hclk (void)
| Enabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_hclk (void)
| Disabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_hclk (void)
| Indicate whether the clock for security blocks(including AES, PKC, Present, HMAC) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_sim_hclk (void)
| Enabling force to turn off the clock for SIM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_sim_hclk (void)
| Disabling force to turn off the clock for SIM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_sim_hclk (void)
| Indicate whether the clock for SIM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_htb_hclk (void)
| Enabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_htb_hclk (void)
| Disabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_htb_hclk (void)
| Indicate whether the clock for Hopping Table is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rom_hclk (void)
| Enabling force to turn off the clock for ROM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rom_hclk (void)
| Disabling force to turn off the clock for ROM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rom_hclk (void)
| Indicate whether the clock for ROM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_snsadc_hclk (void)
| Enabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_snsadc_hclk (void)
| Disabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_snsadc_hclk (void)
| Indicate whether the clock for SNSADC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_gpio_hclk (void)
| Enabling force to turn off the clock for GPIO. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_gpio_hclk (void)
| Disabling force to turn off the clock for GPIO. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_gpio_hclk (void)
| Indicate whether the clock for GPIO is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ble_brg_hclk (void)
| Enabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ble_brg_hclk (void)
| Disabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ble_brg_hclk (void)
| Indicate whether the clock for BLE Bridge is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_apb_sub_hclk (void)
| Enabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_apb_sub_hclk (void)
| Disabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_apb_sub_hclk (void)
| Indicate whether the clock for APB Subsystem is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_serial_hclk (void)
| Enabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_serial_hclk (void)
| Disabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_serial_hclk (void)
| Indicate whether the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_usb_hclk (void)
| Enabling force to turn off the clock for USB. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_usb_hclk (void)
| Disabling force to turn off the clock for USB. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_usb_hclk (void)
| Indicate whether the clock for USB is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aon_mcusub_hclk (void)
| Enabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aon_mcusub_hclk (void)
| Disabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aon_mcusub_hclk (void)
| Indicate whether the clock for AON_MUCSUB is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_hclk (void)
| Enabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_hclk (void)
| Disabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_hclk (void)
| Indicate whether the clock for XQSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_sram_hclk (void)
| Enabling force to turn off the clock for SRAM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_sram_hclk (void)
| Disabling force to turn off the clock for SRAM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_sram_hclk (void)
| Indicate whether the clock for SRAM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart0_hclk (void)
| Enabling force to turn off the clock for UART0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart0_hclk (void)
| Disabling force to turn off the clock for UART0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart0_hclk (void)
| Indicate whether the clock for UART0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart1_hclk (void)
| Enabling force to turn off the clock for UART1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart1_hclk (void)
| Disabling force to turn off the clock for UART1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart1_hclk (void)
| Indicate whether the clock for UART1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart2_hclk (void)
| Enabling force to turn off the clock for UART2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart2_hclk (void)
| Disabling force to turn off the clock for UART2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart2_hclk (void)
| Indicate whether the clock for UART2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart3_hclk (void)
| Enabling force to turn off the clock for UART3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart3_hclk (void)
| Disabling force to turn off the clock for UART3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart3_hclk (void)
| Indicate whether the clock for UART3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart4_hclk (void)
| Enabling force to turn off the clock for UART4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart4_hclk (void)
| Disabling force to turn off the clock for UART4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart4_hclk (void)
| Indicate whether the clock for UART4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart5_hclk (void)
| Enabling force to turn off the clock for UART5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart5_hclk (void)
| Disabling force to turn off the clock for UART5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart5_hclk (void)
| Indicate whether the clock for UART5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c0_hclk (void)
| Enabling force to turn off the clock for I2C0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c0_hclk (void)
| Disabling force to turn off the clock for I2C0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c0_hclk (void)
| Indicate whether the clock for I2C0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c1_hclk (void)
| Enabling force to turn off the clock for I2C1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c1_hclk (void)
| Disabling force to turn off the clock for I2C1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c1_hclk (void)
| Indicate whether the clock for I2C1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c2_hclk (void)
| Enabling force to turn off the clock for I2C2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c2_hclk (void)
| Disabling force to turn off the clock for I2C2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c2_hclk (void)
| Indicate whether the clock for I2C2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c3_hclk (void)
| Enabling force to turn off the clock for I2C3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c3_hclk (void)
| Disabling force to turn off the clock for I2C3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c3_hclk (void)
| Indicate whether the clock for I2C3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c4_hclk (void)
| Enabling force to turn off the clock for I2C4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c4_hclk (void)
| Disabling force to turn off the clock for I2C4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c4_hclk (void)
| Indicate whether the clock for I2C4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c5_hclk (void)
| Enabling force to turn off the clock for I2C5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c5_hclk (void)
| Disabling force to turn off the clock for I2C5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c5_hclk (void)
| Indicate whether the clock for I2C5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spim_hclk (void)
| Enabling force to turn off the clock for SPIM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spim_hclk (void)
| Disabling force to turn off the clock for SPIM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spim_hclk (void)
| Indicate whether the clock for SPIM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spis_hclk (void)
| Enabling force to turn off the clock for SPIS. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spis_hclk (void)
| Disabling force to turn off the clock for SPIS. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spis_hclk (void)
| Indicate whether the clock for SPIS is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi0_hclk (void)
| Enabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi0_hclk (void)
| Disabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi0_hclk (void)
| Indicate whether the clock for QSPI0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi1_hclk (void)
| Enabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi1_hclk (void)
| Disabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi1_hclk (void)
| Indicate whether the clock for QSPI1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi2_hclk (void)
| Enabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi2_hclk (void)
| Disabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi2_hclk (void)
| Indicate whether the clock for QSPI2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_m_hclk (void)
| Enabling force to turn off the clock for I2S master. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_m_hclk (void)
| Disabling force to turn off the clock for I2S master. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_m_hclk (void)
| Indicate whether the clock for I2S master is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_s_p_hclk (void)
| Enabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_s_p_hclk (void)
| Disabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_s_p_hclk (void)
| Indicate whether the clock for I2S slave is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dspi_hclk (void)
| Enabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dspi_hclk (void)
| Disabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dspi_hclk (void)
| Indicate whether the clock for DSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pdm_hclk (void)
| Enabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pdm_hclk (void)
| Disabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pdm_hclk (void)
| Indicate whether the clock for PDM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_div4_pclk (void)
| Enabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_div4_pclk (void)
| Disabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_div4_pclk (void)
| Indicate whether the div4 clock for security blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xf_xqspi_div4_pclk (void)
| Enabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xf_xqspi_div4_pclk (void)
| Disabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xf_xqspi_div4_pclk (void)
| Indicate whether the div4 clock for xf qspi blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm0_hclk (void)
| Enabling force to turn off the clock for PWM0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm0_hclk (void)
| Disabling force to turn off the clock for PWM0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm0_hclk (void)
| Indicate whether the clock for PWM0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm1_hclk (void)
| Enabling force to turn off the clock for PWM1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm1_hclk (void)
| Disabling force to turn off the clock for PWM1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm1_hclk (void)
| Indicate whether the clock for PWM1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_vttbl_hclk (void)
| Enabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_vttbl_hclk (void)
| Disabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_vttbl_hclk (void)
| Indicate whether the clock for VTTBL is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_psram_pclk (void)
| Enabling force to turn off the clock for PSRAM ctrl. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_psram_pclk (void)
| Disabling force to turn off the clock for PSRAM ctrl. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_psram_pclk (void)
| Indicate whether the clock for PSRAM ctrl is forced to close. More...
__STATIC_INLINE void | ll_cgc_set_mcu_periph_low_power (uint32_t clk_mask)
| Some peripherals has low power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_get_mcu_periph_low_power (void)
| Return to clock blocks that has low power feature. More...
__STATIC_INLINE void | ll_cgc_enable_uart_sclk_low_power (void)
| Enable uart sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_sclk_low_power (void)
| Disable uart sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_sclk_low_power (void)
| Indicate whether the uart sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart_pclk_low_power (void)
| Enable uart pclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_pclk_low_power (void)
| Disable uart pclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_pclk_low_power (void)
| Indicate whether the uart pclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_low_power (void)
| Enable i2s low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_low_power (void)
| Disable i2s low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_low_power (void)
| Indicate whether the i2s low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spim_sclk_low_power (void)
| Enable spim sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spim_sclk_low_power (void)
| Disable spim sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spim_sclk_low_power (void)
| Indicate whether the spim sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spis_sclk_low_power (void)
| Enable spis sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spis_sclk_low_power (void)
| Disable spis sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spis_sclk_low_power (void)
| Indicate whether the spis sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c_sclk_low_power (void)
| Enable i2c sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2c_sclk_low_power (void)
| Disable i2c sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c_sclk_low_power (void)
| Indicate whether the i2c sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim_low_power (void)
| Enable QSPIM low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_qspim_low_power (void)
| Disable QSPIM low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim_low_power (void)
| Indicate whether the QSPIM low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_sync_bus_low_power (void)
| Enable AHB2APB bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_sync_bus_low_power (void)
| Disable AHB2APB bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_sync_bus_low_power (void)
| Indicate whether the AHB2APB bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_async_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_async_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_async_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart0_slp_wfi (void)
| Enable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart0_slp_wfi (void)
| Disable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart0_slp_wfi (void)
| Indicate whether turn UART0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart1_slp_wfi (void)
| Enable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart1_slp_wfi (void)
| Disable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart1_slp_wfi (void)
| Indicate whether turn UART1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart2_slp_wfi (void)
| Enable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart2_slp_wfi (void)
| Disable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart2_slp_wfi (void)
| Indicate whether turn UART2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart3_slp_wfi (void)
| Enable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart3_slp_wfi (void)
| Disable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart3_slp_wfi (void)
| Indicate whether turn UART3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart4_slp_wfi (void)
| Enable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart4_slp_wfi (void)
| Disable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart4_slp_wfi (void)
| Indicate whether turn UART4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart5_slp_wfi (void)
| Enable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart5_slp_wfi (void)
| Disable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart5_slp_wfi (void)
| Indicate whether turn UART5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c0_slp_wfi (void)
| Enable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c0_slp_wfi (void)
| Disable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c0_slp_wfi (void)
| Indicate whether turn I2C0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c1_slp_wfi (void)
| Enable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c1_slp_wfi (void)
| Disable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c1_slp_wfi (void)
| Indicate whether turn I2C1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c2_slp_wfi (void)
| Enable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c2_slp_wfi (void)
| Disable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c2_slp_wfi (void)
| Indicate whether turn I2C2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c3_slp_wfi (void)
| Enable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c3_slp_wfi (void)
| Disable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c3_slp_wfi (void)
| Indicate whether turn I2C3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c4_slp_wfi (void)
| Enable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c4_slp_wfi (void)
| Disable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c4_slp_wfi (void)
| Indicate whether turn I2C4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c5_slp_wfi (void)
| Enable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c5_slp_wfi (void)
| Disable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c5_slp_wfi (void)
| Indicate whether turn I2C5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_m_slp_wfi (void)
| Enable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_m_slp_wfi (void)
| Disable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_m_slp_wfi (void)
| Indicate whether turn I2S_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_s_slp_wfi (void)
| Enable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_s_slp_wfi (void)
| Disable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_s_slp_wfi (void)
| Indicate whether turn I2S_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_m_slp_wfi (void)
| Enable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_m_slp_wfi (void)
| Disable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_m_slp_wfi (void)
| Indicate whether turn SPI_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_s_slp_wfi (void)
| Enable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_s_slp_wfi (void)
| Disable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_s_slp_wfi (void)
| Indicate whether turn SPI_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm0_slp_wfi (void)
| Enable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm0_slp_wfi (void)
| Disable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm0_slp_wfi (void)
| Indicate whether turn pwm0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm1_slp_wfi (void)
| Enable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm1_slp_wfi (void)
| Disable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm1_slp_wfi (void)
| Indicate whether turn pwm1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim0_slp_wfi (void)
| Enable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim0_slp_wfi (void)
| Disable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim0_slp_wfi (void)
| Indicate whether turn QSPIM0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim1_slp_wfi (void)
| Enable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim1_slp_wfi (void)
| Disable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim1_slp_wfi (void)
| Indicate whether turn QSPIM1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim2_slp_wfi (void)
| Enable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim2_slp_wfi (void)
| Disable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim2_slp_wfi (void)
| Indicate whether turn QSPIM2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_dspi_slp_wfi (void)
| Enable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_dspi_slp_wfi (void)
| Disable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_dspi_slp_wfi (void)
| Indicate whether turn DSPI off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pdm_slp_wfi (void)
| Enable turn PDM off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pdm_slp_wfi (void)
| Disable turn PDM off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pdm_slp_wfi (void)
| Indicate whether turn PDM off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_secu (uint32_t clk_mask)
| Individual block's clock control inside security system which was forced to turn off (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_secu (void)
| Return to clock blocks that was forcibly closed inside security system. More...
__STATIC_INLINE void | ll_cgc_set_slp_off_hclk_secu (uint32_t clk_mask)
| Some security blocks automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_get_slp_off_secu (void)
| Return to security clock blocks that is turned off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aes_hclk (void)
| Enabling force to turn off the clock for AES. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aes_hclk (void)
| Disabling force to turn off the clock for AES. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aes_hclk (void)
| Indicate whether the clock for AES is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_hmac_hclk (void)
| Enabling force to turn off the clock for HMAC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_hmac_hclk (void)
| Disabling force to turn off the clock for HMAC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_hmac_hclk (void)
| Indicate whether the clock for HMAC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pkc_hclk (void)
| Enabling force to turn off the clock for PKC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pkc_hclk (void)
| Disabling force to turn off the clock for PKC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pkc_hclk (void)
| Indicate whether the clock for PKC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_present_hclk (void)
| Enabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_present_hclk (void)
| Disabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_present_hclk (void)
| Indicate whether the clock for PRESENT is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ramkey_hclk (void)
| Enabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ramkey_hclk (void)
| Disabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ramkey_hclk (void)
| Indicate whether the clock for RAMKEY is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rng_hclk (void)
| Enabling force to turn off the clock for RNG. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rng_hclk (void)
| Disabling force to turn off the clock for RNG. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rng_hclk (void)
| Indicate whether the clock for RNG is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_efuse_hclk (void)
| Enabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_efuse_hclk (void)
| Disabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_efuse_hclk (void)
| Indicate whether the clock for EFUSE is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aes_hclk (void)
| Enable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aes_hclk (void)
| Disable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aes_hclk (void)
| Indicate whether the AES automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_hmac_hclk (void)
| Enable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_hmac_hclk (void)
| Disable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_hmac_hclk (void)
| Indicate whether the HMAC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pkc_hclk (void)
| Enable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pkc_hclk (void)
| Disable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pkc_hclk (void)
| Indicate whether the PKC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_present_hclk (void)
| Enable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_present_hclk (void)
| Disable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_present_hclk (void)
| Indicate whether the PRESENT automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ramkey_hclk (void)
| Enable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ramkey_hclk (void)
| Disable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ramkey_hclk (void)
| Indicate whether the RAMKEY automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rng_hclk (void)
| Enable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rng_hclk (void)
| Disable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rng_hclk (void)
| Indicate whether the RNG automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_efuse_hclk (void)
| Enable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_efuse_hclk (void)
| Disable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_efuse_hclk (void)
| Indicate whether the EFUSE automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_set_misc_clk (uint32_t clk_mask)
| Some MISC_CLK blocks turn off clock. More...
__STATIC_INLINE uint32_t | ll_cgc_get_misc_clk (void)
| Return to MISC_CLK clock blocks that is turned off. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_sck (void)
| Enable XQSPI SCK CLK turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_sck (void)
| Disable XQSPI SCK CLK turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_sck (void)
| Indicate whether the XQSPI SCK CLK automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dma0_hclk (void)
| Enable DMA0 turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dma0_hclk (void)
| Disable DMA0 turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dma0_hclk (void)
| Indicate whether the DMA0 automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dma1_hclk (void)
| Enable DMA1 turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dma1_hclk (void)
| Disable DMA1 turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dma1_hclk (void)
| Indicate whether the DMA1 automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dma2_hclk (void)
| Enable DMA2 turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dma2_hclk (void)
| Disable DMA2 turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dma2_hclk (void)
| Indicate whether the DMA2 automatic turn off clock is enabled. More...

## Detailed Description

Header file containing functions prototypes of CGC LL library.

Author
  BLE Driver Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file gr55xx_ll_cgc.h.