Modules
Shelf Label AP Client (ESLS_C)
BLE Services

Electronic Shelf Label Client module. More...

## Modules
| Defines
| Enumerations
| Structures
| DEF Typedefs
| Functions

## Detailed Description

Electronic Shelf Label Client module.

The Electronic Shelf Label Client contains the APIs and types, which can be used by the application to discovery of Heart Rate Service of peer and interact with it.

The application must provide an event handler to register, then call esls_client_init(). After Heart Rate Service Client discoveries peer Electronic Shelf Label Service, application can call esls_c_ctrl_point_notify_set(), then will config peer service resource, also can call esls_c_esl_key_set() and esls_c_disp_info_read() to set device key, or get device infor.