### - a -

- ADC_CFG_REG_DEFAULT : gr55xx_hal_adc.h
- ADC_DEFAULT_CONFIG : gr55xx_hal_adc.h
- ADC_INPUT_DIFFERENTIAL : gr55xx_hal_adc.h
- ADC_INPUT_SINGLE : gr55xx_hal_adc.h
- ADC_INPUT_SRC_BAT : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO0 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO1 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO2 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO3 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO4 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO5 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO6 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO7 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_REF : gr55xx_hal_adc.h
- ADC_INPUT_SRC_TMP : gr55xx_hal_adc.h
- ADC_REF_SRC_BUF_INT : gr55xx_hal_adc.h
- ADC_REF_SRC_IO0 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO1 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO2 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO3 : gr55xx_hal_adc.h
- ADC_REF_VALUE_0P8 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P2 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P6 : gr55xx_hal_adc.h
- ADC_REF_VALUE_2P0 : gr55xx_hal_adc.h
- AES_BLOCK_MAX : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BITS : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BYTES : gr55xx_hal_aes.h
- AES_BLOCKSIZE_WORDS : gr55xx_hal_aes.h
- AES_CHAININGMODE_CBC : gr55xx_hal_aes.h
- AES_CHAININGMODE_ECB : gr55xx_hal_aes.h
- AES_FLAG_DATAREADY : gr55xx_hal_aes.h
- AES_FLAG_DMA_DONE : gr55xx_hal_aes.h
- AES_FLAG_DMA_ERR : gr55xx_hal_aes.h
- AES_FLAG_KEY_VALID : gr55xx_hal_aes.h
- AES_IT_DONE : gr55xx_hal_aes.h
- AES_KEYSIZE_128BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_192BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_256BITS : gr55xx_hal_aes.h
- AES_OPERATION_MODE_DECRYPT : gr55xx_hal_aes.h
- AES_OPERATION_MODE_ENCRYPT : gr55xx_hal_aes.h
- AGS_CHAR_FULL : ags.h
- AGS_CHAR_MANDATORY : ags.h
- AGS_CONNECTION_MAX : ags.h
- AGS_HEADER_ACK_PAYLOAD_LEN : ags.h
- AGS_HEADER_ACK_RES_1 : ags.h
- AGS_HEADER_ACK_RES_2 : ags.h
- AGS_HEADER_FIRST_RES : ags.h
- AGS_PAIR_ADV_FLAG : ags.h
- AGS_RECONNECT_ADV_FLAG : ags.h
- AGS_RX_VAL_LEN_MAX : ags.h
- AGS_SERVICE_UUID : ags.h
- AGS_TX_VAL_LEN_MAX : ags.h
- ALL_DEVICES_BACKUP : gr55xx_hal_pwr_mgmt.h
- ALL_DEVICES_SLEEP : gr55xx_hal_pwr_mgmt.h
- AMS_ATTR_DISPLAY_UUID : ams_c.h
- AMS_ATTR_UPDATE_UUID : ams_c.h
- AMS_C_ATTR_COUNT_MAX : ams_c.h
- AMS_C_CONNECTION_MAX : ams_c.h
- AMS_C_TRUNCATED_FLAG : ams_c.h
- AMS_CMD_UUID : ams_c.h
- AMS_SRVC_UUID : ams_c.h
- ANCS_ATTR : ancs_protocol.h
- ANCS_ATTR_MAXLEN : ancs_protocol.h
- ANCS_C_CONNECTION_MAX : ancs_c.h
- ANCS_CONTROL_POINT_UUID : ancs_c.h
- ANCS_DATA_SOURCE_UUID : ancs_c.h
- ANCS_NTF_SOURCE_UUID : ancs_c.h
- ANCS_SRVC_UUID : ancs_c.h
- ANS_ALERT_NTF_CTRL_PT_VAL_LEN : ans.h
- ANS_ALL_CAT_SUP : ans.h
- ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN : ans_c.h
- ANS_C_ALL_CAT_SUP : ans_c.h
- ANS_C_CALL_SUP : ans_c.h
- ANS_C_CONNECTION_MAX : ans_c.h
- ANS_C_EMAIL_SUP : ans_c.h
- ANS_C_ERROR_CMD_NOT_SUP : ans_c.h
- ANS_C_HG_PRIO_ALERT_SUP : ans_c.h
- ANS_C_INSTANT_MES : ans_c.h
- ANS_C_MISSED_CALL_SUP : ans_c.h
- ANS_C_NEWS_SUP : ans_c.h
- ANS_C_SCHEDULE_SUP : ans_c.h
- ANS_C_SMPL_ALERT_SUP : ans_c.h
- ANS_C_SMS_MMS_SUP : ans_c.h
- ANS_C_UTF_8_STR_LEN_MAX : ans_c.h
- ANS_C_VOICE_MAIL_SUP : ans_c.h
- ANS_CALL_SUP : ans.h
- ANS_CONNECTION_MAX : ans.h
- ANS_EMAIL_SUP : ans.h
- ANS_ERROR_CMD_NOT_SUP : ans.h
- ANS_HG_PRIO_ALERT_SUP : ans.h
- ANS_INSTANT_MES : ans.h
- ANS_MISSED_CALL_SUP : ans.h
- ANS_NEWS_ALERT_VAL_LEN : ans.h
- ANS_NEWS_SUP : ans.h
- ANS_SCHEDULE_SUP : ans.h
- ANS_SMPL_ALERT_SUP : ans.h
- ANS_SMS_MMS_SUP : ans.h
- ANS_SUP_NEW_ALERT_CAT_VAL_LEN : ans.h
- ANS_SUP_UNREAD_ALERT_CAT_VAL_LEN : ans.h
- ANS_UNREAD_ALERT_STA_VAL_LEN : ans.h
- ANS_UTF_8_STR_LEN_MAX : ans.h
- ANS_VOICE_MAIL_SUP : ans.h
- AON_GPIO_DEFAULT_CONFIG : gr55xx_hal_aon_gpio.h
- AON_GPIO_INPUT_TYPE_CMOS : gr55xx_hal_aon_gpio.h
- AON_GPIO_INPUT_TYPE_SCHMITT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_INOUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_INPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_BOTH_EDGE : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_FALLING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_LOW : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_RISING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_MUX : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_NONE : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_OUTPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MUX_0 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_1 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_2 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_3 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_4 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_5 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_6 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_7 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_8 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_NOPULL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_0 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_1 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_2 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_3 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_4 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_5 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_6 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_7 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_ALL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_MASK : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLDOWN : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLUP : gr55xx_hal_aon_gpio.h
- AON_GPIO_SPEED_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_SPEED_MEDIUM : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_LOW : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_MEDIUM : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_ULTRA : gr55xx_hal_aon_gpio.h
- AON_WDT_REG_READ : gr55xx_ll_aon_wdt.h
- AP_SYNC_KEY_MATERIAL_LEN : esls.h
- app_adc_dma_conversion_async : app_adc_dma.h
- app_adc_dma_multi_channel_conversion_async : app_adc_dma.h
- APP_AON_IO_PIN_ALL : app_io.h
- APP_BOD_DISABLE : app_bod.h
- APP_BOD_ENABLE : app_bod.h
- APP_BOD_EVENT_DISABLE : app_bod.h
- APP_BOD_EVENT_ENABLE : app_bod.h
- APP_BOD_EVENT_LEVEL_0 : app_bod.h
- APP_BOD_EVENT_LEVEL_1 : app_bod.h
- APP_BOD_EVENT_LEVEL_2 : app_bod.h
- APP_BOD_EVENT_LEVEL_3 : app_bod.h
- APP_BOD_EVENT_LEVEL_4 : app_bod.h
- APP_BOD_EVENT_LEVEL_5 : app_bod.h
- APP_BOD_EVENT_LEVEL_6 : app_bod.h
- APP_BOD_EVENT_LEVEL_7 : app_bod.h
- APP_BOD_STATIC_DISABLE : app_bod.h
- APP_BOD_STATIC_ENABLE : app_bod.h
- APP_DRIVER_ADC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_AES_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_COMP_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DMA_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DUAL_TIM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_GR5332X : app_drv_config.h
- APP_DRIVER_GR5405 : app_drv_config.h
- APP_DRIVER_GR551X : app_drv_config.h
- APP_DRIVER_GR5525X : app_drv_config.h
- APP_DRIVER_GR5526X : app_drv_config.h
- APP_DRIVER_HMAC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2C_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2S_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_ISO7816_WAKEUP_PRIORITY : app_drv_config.h
- app_driver_mutex_deinit : app_rtos_cfg.h
- app_driver_mutex_init : app_rtos_cfg.h
- app_driver_mutex_pend : app_rtos_cfg.h
- app_driver_mutex_post : app_rtos_cfg.h
- APP_DRIVER_PKC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_PWM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_QSPI_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_RNG_WAKEUP_PRIORITY : app_drv_config.h
- app_driver_sem_deinit : app_rtos_cfg.h
- app_driver_sem_init : app_rtos_cfg.h
- app_driver_sem_pend : app_rtos_cfg.h
- app_driver_sem_post : app_rtos_cfg.h
- app_driver_sem_post_from_isr : app_rtos_cfg.h
- APP_DRIVER_SPI_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_TIM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_UART_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRV_ASSERT : app_drv.h
- APP_DRV_ASSERT_ENABLE : app_drv_config.h
- APP_DRV_DEPRECATED : app_drv.h
- APP_DRV_ERR_BUSY : app_drv_error.h
- APP_DRV_ERR_CODE_CHECK : app_drv_error.h
- APP_DRV_ERR_HAL : app_drv_error.h
- APP_DRV_ERR_INVALID_ID : app_drv_error.h
- APP_DRV_ERR_INVALID_INIT : app_drv_error.h
- APP_DRV_ERR_INVALID_MODE : app_drv_error.h
- APP_DRV_ERR_INVALID_PARAM : app_drv_error.h
- APP_DRV_ERR_INVALID_TYPE : app_drv_error.h
- APP_DRV_ERR_NOT_INIT : app_drv_error.h
- APP_DRV_ERR_POINTER_NULL : app_drv_error.h
- APP_DRV_ERR_TIMEOUT : app_drv_error.h
- APP_DRV_LOG_ERR : app_drv.h
- APP_DRV_LOG_INFO : app_drv.h
- APP_DRV_LOG_INTERFACE : app_drv_config.h
- APP_DRV_LOG_LEVEL : app_drv_config.h
- APP_DRV_LOG_WARN : app_drv.h
- APP_DRV_MAX_TIMEOUT : app_drv.h
- APP_DRV_MUTEX_DECL : app_rtos_cfg.h
- APP_DRV_MUTEX_STATIC : app_rtos_cfg.h
- APP_DRV_NEVER_TIMEOUT : app_drv.h
- APP_DRV_SEM_DECL : app_rtos_cfg.h
- APP_DRV_SEM_STATIC : app_rtos_cfg.h
- APP_DRV_SUCCESS : app_drv_error.h
- APP_DSPI_PIN_DISABLE : app_dspi.h
- APP_DSPI_PIN_ENABLE : app_dspi.h
- APP_DVR_LOG_LVL_ERR : app_drv_config.h
- APP_DVR_LOG_LVL_INFO : app_drv_config.h
- APP_DVR_LOG_LVL_NONE : app_drv_config.h
- APP_DVR_LOG_LVL_WARN : app_drv_config.h
- APP_IO_DEFAULT_CONFIG : app_io.h
- APP_IO_MUX : app_io.h
- APP_IO_PIN_0 : app_io.h
- APP_IO_PIN_1 : app_io.h
- APP_IO_PIN_10 : app_io.h
- APP_IO_PIN_11 : app_io.h
- APP_IO_PIN_12 : app_io.h
- APP_IO_PIN_13 : app_io.h
- APP_IO_PIN_14 : app_io.h
- APP_IO_PIN_15 : app_io.h
- APP_IO_PIN_16 : app_io.h
- APP_IO_PIN_17 : app_io.h
- APP_IO_PIN_18 : app_io.h
- APP_IO_PIN_19 : app_io.h
- APP_IO_PIN_2 : app_io.h
- APP_IO_PIN_20 : app_io.h
- APP_IO_PIN_21 : app_io.h
- APP_IO_PIN_22 : app_io.h
- APP_IO_PIN_23 : app_io.h
- APP_IO_PIN_24 : app_io.h
- APP_IO_PIN_25 : app_io.h
- APP_IO_PIN_26 : app_io.h
- APP_IO_PIN_27 : app_io.h
- APP_IO_PIN_28 : app_io.h
- APP_IO_PIN_29 : app_io.h
- APP_IO_PIN_3 : app_io.h
- APP_IO_PIN_30 : app_io.h
- APP_IO_PIN_31 : app_io.h
- APP_IO_PIN_4 : app_io.h
- APP_IO_PIN_5 : app_io.h
- APP_IO_PIN_6 : app_io.h
- APP_IO_PIN_7 : app_io.h
- APP_IO_PIN_8 : app_io.h
- APP_IO_PIN_9 : app_io.h
- APP_IO_PIN_ALL : app_io.h
- APP_IO_PIN_MASK : app_io.h
- APP_IO_PINS_0_15 : app_io.h
- APP_IO_PINS_0_7 : app_io.h
- APP_IO_PINS_16_31 : app_io.h
- APP_MSIO_IO_PIN_ALL : app_io.h
- APP_PARAM_ID_ACTIVITY_MOVE_CONFIG : nvds_tag.h
- APP_PARAM_ID_RF_LPCLK_DRIFT : nvds_tag.h
- APP_PARAM_ID_RF_XO_OFFSET : nvds_tag.h
- APP_PWM_PIN_DISABLE : app_pwm.h
- APP_PWM_PIN_ENABLE : app_pwm.h
- APP_QSPI_PIN_DISABLE : app_qspi.h
- APP_QSPI_PIN_ENABLE : app_qspi.h
- APP_RTC_ALARM_DISABLE_ALL : app_rtc.h
- APP_RTC_ALARM_DISABLE_DATE : app_rtc.h
- APP_RTC_ALARM_DISABLE_TICK : app_rtc.h
- APP_SLEEP_CB_MAX : app_pwr_mgmt.h
- APP_SPI_PIN_DISABLE : app_spi.h
- APP_SPI_PIN_ENABLE : app_spi.h
- AUTO_RELOAD : gr55xx_hal_rtc.h