Public Attributes | List of all members
ble_gap_ranging_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

ranging parameter. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | channel_sequence [BLE_GAP_MAX_GDX_RANGING_CH]
| ranging channel sequence More...
uint8_t | channel_num
| Number of channel to be collected. More...

## Detailed Description

ranging parameter.

Definition at line 773 of file ble_gapc.h.

## Member Data Documentation

## ◆ channel_num

uint8_t ble_gap_ranging_param_t::channel_num

Number of channel to be collected.

Definition at line 778 of file ble_gapc.h.

## ◆ channel_sequence

uint8_t ble_gap_ranging_param_t::channel_sequence[BLE_GAP_MAX_GDX_RANGING_CH]

ranging channel sequence

Definition at line 776 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h