Functions
Functions
Peripheral Driver » HAL Driver » HAL_Delay

## Functions
void | delay_us (uint32_t number_of_us)
| Function for delaying execution for number of microseconds. GR55xxx is based on Cortex-M4, and this function is based on Data Watchpoint and Trace (DWT) unit. More...
void | delay_ms (uint32_t number_of_ms)
| Function for delaying execution for number of milliseconds. GR55xxx is based on Cortex-M4, and this function is based on Data Watchpoint and Trace (DWT) unit. More...

## Detailed Description

## Function Documentation

## ◆ delay_ms()

void delay_ms | ( | uint32_t | number_of_ms | ) |

Function for delaying execution for number of milliseconds. GR55xxx is based on Cortex-M4, and this function is based on Data Watchpoint and Trace (DWT) unit.

Parameters

  [in] | number_of_ms | number of milliseconds

## ◆ delay_us()

void delay_us | ( | uint32_t | number_of_us | ) |

Function for delaying execution for number of microseconds. GR55xxx is based on Cortex-M4, and this function is based on Data Watchpoint and Trace (DWT) unit.

Parameters

  [in] | number_of_us | number of microseconds