Macros
Test Mode
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_NORMAL_MODE 0x00000000UL
#define | LL_QSPI_TEST_MODE (1UL << QSPI_CTRL0_SRL_Pos)
#define | LL_SPI_NORMAL_MODE 0x00000000UL
#define | LL_SPI_TEST_MODE (1UL << SPI_CTRL0_SHIFT_REG_LOOP_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_NORMAL_MODE

#define LL_QSPI_NORMAL_MODE 0x00000000UL

Normal mode for SPI transfer

Definition at line 443 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_TEST_MODE

#define LL_QSPI_TEST_MODE (1UL << QSPI_CTRL0_SRL_Pos)

Test mode for SPI transfer: Rx and Tx connected inside

Definition at line 444 of file gr55xx_ll_qspi.h.

## ◆ LL_SPI_NORMAL_MODE

#define LL_SPI_NORMAL_MODE 0x00000000UL

Normal mode for SPI transfer

Definition at line 245 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_TEST_MODE

#define LL_SPI_TEST_MODE (1UL << SPI_CTRL0_SHIFT_REG_LOOP_POS)

Test mode for SPI transfer: Rx and Tx connected inside

Definition at line 246 of file gr55xx_ll_spi.h.