Macros
Bits phase for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants

## Macros
#define | QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE LL_QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE
#define | QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE LL_QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE

#define QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE LL_QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE

Disable Bits phase.

Definition at line 662 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE

#define QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE LL_QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE

Enable Bits phase.

Definition at line 661 of file gr55xx_hal_qspi.h.