Public Attributes | List of all members
ble_gap_connless_iq_sample_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Set connectionless IQ sampling enable parameter. More...

`#include <ble_gapm.h>`

## Public Attributes
uint8_t | slot_dur
uint8_t | max_smaple_cte
uint8_t | antenna_num
uint8_t * | antenna_id

## Detailed Description

Set connectionless IQ sampling enable parameter.

Definition at line 713 of file ble_gapm.h.

## Member Data Documentation

## ◆ antenna_id

uint8_t* ble_gap_connless_iq_sample_param_t::antenna_id

List of Antenna IDs in the pattern.

Definition at line 719 of file ble_gapm.h.

## ◆ antenna_num

uint8_t ble_gap_connless_iq_sample_param_t::antenna_num

The number of antenna IDs in the pattern (range 0x02 to 0x4B).

Definition at line 718 of file ble_gapm.h.

## ◆ max_smaple_cte

uint8_t ble_gap_connless_iq_sample_param_t::max_smaple_cte

The maximum number of CTE to sample and report in each periodic advertising interval (range 0x00 to 0x10). 0x00: Sample and report all available CTE.

Definition at line 716 of file ble_gapm.h.

## ◆ slot_dur

uint8_t ble_gap_connless_iq_sample_param_t::slot_dur

The slot duration for IQ sampling, see enum gap_slot_dur_type.

Definition at line 715 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h