Macros
Turn the peripherals off during WFI/WFE
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART2
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART3
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SM
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SS
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM2
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_DSPI
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PDM
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C2
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C3
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x007C3F0FUL)
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x007FFF0FUL)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_DSPI

Turn the dspi off during WFI/WFE

Definition at line 198 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0

Turn the i2c0 off during WFI/WFE

Definition at line 200 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1

Turn the i2c1 off during WFI/WFE

Definition at line 201 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C2

Turn the i2c0 off during WFI/WFE

Definition at line 202 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C3

Turn the i2c1 off during WFI/WFE

Definition at line 203 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SM

Turn the i2s_m off during WFI/WFE

Definition at line 189 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SS

Turn the i2s_s off during WFI/WFE

Definition at line 190 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PDM

Turn the pdm off during WFI/WFE

Definition at line 199 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0

Turn the pwm0 off during WFI/WFE

Definition at line 193 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1

Turn the pwm1 off during WFI/WFE

Definition at line 194 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM0

Turn the qspim0 off during WFI/WFE

Definition at line 195 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM1

Turn the qspim1 off during WFI/WFE

Definition at line 196 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM2

Turn the qspim2 off during WFI/WFE

Definition at line 197 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM

Turn the spi_m off during WFI/WFE

Definition at line 191 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS

Turn the spi_s off during WFI/WFE

Definition at line 192 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0

Turn the uart0 off during WFI/WFE

Definition at line 185 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1

Turn the uart1 off during WFI/WFE

Definition at line 186 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART2

Turn the uart2 off during WFI/WFE

Definition at line 187 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART3

Turn the uart3 off during WFI/WFE

Definition at line 188 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x007FFF0FUL)

Serial blocks

Definition at line 206 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x007C3F0FUL)

Serial blocks

Definition at line 205 of file gr55xx_ll_cgc.h.