Macros
MicroWire Control
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL
#define | LL_QSPI_MICROWIRE_HANDSHAKE_EN (1UL << QSPI_MWC_MHS_Pos)
#define | LL_QSPI_MICROWIRE_RX 0x00000000UL
#define | LL_QSPI_MICROWIRE_TX (1UL << QSPI_MWC_MDD_Pos)
#define | LL_QSPI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL
#define | LL_QSPI_MICROWIRE_SEQUENTIAL (1UL << QSPI_MWC_MWMOD_Pos)
#define | LL_SPI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL
#define | LL_SPI_MICROWIRE_HANDSHAKE_EN (1UL << SPI_MW_CTRL_MW_HSG_POS)
#define | LL_SPI_MICROWIRE_RX 0x00000000UL
#define | LL_SPI_MICROWIRE_TX (1UL << SPI_MW_CTRL_MW_DIR_DW_POS)
#define | LL_SPI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL
#define | LL_SPI_MICROWIRE_SEQUENTIAL (1UL << SPI_MW_CTRL_MW_XFE_MODE_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_MICROWIRE_HANDSHAKE_DIS

#define LL_QSPI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL

Enable Handshake for Microwire transfer

Definition at line 488 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MICROWIRE_HANDSHAKE_EN

#define LL_QSPI_MICROWIRE_HANDSHAKE_EN (1UL << QSPI_MWC_MHS_Pos)

Disable Handshake for Microwire transfer

Definition at line 489 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MICROWIRE_NON_SEQUENTIAL

#define LL_QSPI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL

Non-sequential for Microwire transfer

Definition at line 494 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MICROWIRE_RX

#define LL_QSPI_MICROWIRE_RX 0x00000000UL

Rx mode. Rx transfer at Microwire mode

Definition at line 491 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MICROWIRE_SEQUENTIAL

#define LL_QSPI_MICROWIRE_SEQUENTIAL (1UL << QSPI_MWC_MWMOD_Pos)

Sequential for Microwire transfer

Definition at line 495 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MICROWIRE_TX

#define LL_QSPI_MICROWIRE_TX (1UL << QSPI_MWC_MDD_Pos)

Tx mode. Tx transfer at Microwire mode

Definition at line 492 of file gr55xx_ll_qspi.h.

## ◆ LL_SPI_MICROWIRE_HANDSHAKE_DIS

#define LL_SPI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL

Enable Handshake for Microwire transfer

Definition at line 290 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MICROWIRE_HANDSHAKE_EN

#define LL_SPI_MICROWIRE_HANDSHAKE_EN (1UL << SPI_MW_CTRL_MW_HSG_POS)

Disable Handshake for Microwire transfer

Definition at line 291 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MICROWIRE_NON_SEQUENTIAL

#define LL_SPI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL

Non-sequential for Microwire transfer

Definition at line 296 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MICROWIRE_RX

#define LL_SPI_MICROWIRE_RX 0x00000000UL

Rx mode. Rx transfer at Microwire mode

Definition at line 293 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MICROWIRE_SEQUENTIAL

#define LL_SPI_MICROWIRE_SEQUENTIAL (1UL << SPI_MW_CTRL_MW_XFE_MODE_POS)

Sequential for Microwire transfer

Definition at line 297 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MICROWIRE_TX

#define LL_SPI_MICROWIRE_TX (1UL << SPI_MW_CTRL_MW_DIR_DW_POS)

Tx mode. Tx transfer at Microwire mode

Definition at line 294 of file gr55xx_ll_spi.h.