### - c -

- cache_current_state : ble_gattc_evt_cache_update_t
- cache_direct_map_en : _ll_xqspi_init_t , _xqspi_init_t
- cache_flush : _ll_xqspi_init_t , _xqspi_init_t
- cache_mode : _ll_xqspi_init_t , _xqspi_init_t
- cache_size : ble_hci_rx_channel_t
- cache_update : ble_gattc_evt_t
- cache_valid : ble_gattc_evt_cache_update_t
- cal_data_rec_num : cgms_cp_cmd_req_t
- cal_data_record_num : __attribute__
- cal_status : __attribute__
- cal_temp : __attribute__
- cal_value : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- calendar_alarm_callback : _hal_calendar_callback
- calendar_overflow_callback : _hal_calendar_callback
- calendar_tick_callback : _hal_calendar_callback
- carbohydrate : gls_meas_ctx_t
- carbohydrate_id : gls_meas_ctx_t
- cat_id : ans_c_ctrl_pt_t , ans_c_new_alert_t , ans_c_unread_alert_t , ans_ctrl_pt_t , ans_new_alert_t , ans_unread_alert_t
- cat_ids : ans_evt_t
- category_count : ntf_source_pdu_t
- category_id : ntf_source_pdu_t
- cccd : ras_c_read_rsp_t
- cccd_change_handler : bms_init_t , cgms_init_t
- cccd_recovery : ble_gatts_evt_t
- cccd_val : ble_gatts_evt_cccd_rec_t
- cccd_value : ras_ad_set_cccd_info_t
- ce_len : ble_gap_conn_update_param_t , ble_gap_ext_conn_param_t
- cert_list : ble_dis_c_read_rsp_t
- ch_idx : gdx_lcp_config_t
- chaining_mode : _aes_init
- chan_sel_algo : ble_gap_conn_info_t
- channel : _dma_handle , app_dspi_dma_cfg_t , link_node
- channel_a : _ll_pwm_init_t , app_pwm_pin_cfg_t , pwm_init_t
- channel_b : _ll_pwm_init_t , app_pwm_pin_cfg_t , pwm_init_t
- channel_c : _ll_pwm_init_t , app_pwm_pin_cfg_t , pwm_init_t
- channel_idx : ble_gap_connless_iq_report_t , ble_gap_evt_connless_iq_report_t
- channel_n : app_adc_pin_cfg_t
- channel_num : ble_gap_ranging_param_t
- channel_number : app_dma_params_t
- channel_p : app_adc_pin_cfg_t
- channel_sequence : ble_gap_ranging_param_t
- char_decl : attr_cache_info
- char_desc : attr_cache_info
- char_desc_disc : ble_gattc_evt_t
- char_descs : ble_gattc_char_desc_disc_t , ble_gattc_evt_char_desc_disc_t
- char_disc : ble_gattc_evt_t
- char_mask : ags_init_t , bas_init_t , bcs_init_t , bps_init_t , cscs_init_t , cts_init_t , dis_init_t , esls_init_t , gls_init_t , hrs_init_t , hts_init_t , pass_init_t , rscs_init_t , rtus_init_t , uds_init_t , wss_init_t
- char_type : ble_dis_c_read_rsp_t , ras_c_ad_read_ntf_ind_data_t , ras_c_ad_write_req_t , ras_c_ad_write_rsp_t
- chars : ble_gattc_char_disc_t , ble_gattc_evt_char_disc_t
- check_image : dfu_boot_info_t
- check_sum : dfu_boot_info_t , dfu_receive_frame_t
- chip_id : __attribute__ , _efuse_trim0_t
- chip_uid : _efuse_trim0_t
- chnl_map : ble_gap_adv_param_t , ble_gap_adv_prim_cfg_t , ble_gap_conn_info_t
- ci : thscps_test_conn_info_t
- cid : ble_l2cap_evt_sdu_recv_t , ble_l2cap_evt_sdu_send_t , ble_l2cap_lecb_sdu_t , lecb_sdu_send_evt_t
- clk : app_dspi_pin_cfg_t , app_graphics_dc_pins_t , app_pdm_pin_cfg_t , app_qspi_pin_cfg_t , app_spi_pin_cfg_t
- clk_acc : ble_gap_evt_sync_established_t , ble_gap_sync_established_ind_t
- clk_accuracy : ble_gap_evt_connected_t , gap_conn_cmp_t
- clk_div : _ll_iso7816_init , iso7816_init_t
- clock_freq : _calendar_handle , app_graphics_dc_params_t
- clock_mode : _qspi_init_t , _xqspi_init_t , app_graphics_dc_params_t
- clock_phase : _ll_qspi_init_t , _ll_qspi_memorymapped_init_t , _ll_spim_init_t , _ll_spis_init_t , _ll_xqspi_init_t , _spi_init
- clock_polarity : _ll_qspi_init_t , _ll_qspi_memorymapped_init_t , _ll_spim_init_t , _ll_spis_init_t , _ll_xqspi_init_t , _spi_init
- clock_prescaler : _qspi_init_t
- clock_source : _i2s_init , _ll_i2s_init_t
- clock_stretch_en : _qspi_command_t
- cmd_id : ans_c_ctrl_pt_t , ans_ctrl_pt_t , hrrcps_rsp_val_t , thscps_rsp_val_t
- cmd_list : ams_c_evt_t
- cmd_type : dfu_receive_frame_t
- cmp_data_rsp : ras_ctr_pt_rsp_t
- cmp_lost_data_seg_rsp : ras_ctr_pt_rsp_t
- code_copy_mode : dfu_boot_info_t
- comm_interval_in_minutes : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- command : app_graphics_dc_cmd_t
- comments : dfu_image_info_t
- commit_id : sdk_version_t
- comp_env : app_comp_params_t
- comp_msp_deinit : _hal_comp_callback
- comp_msp_init : _hal_comp_callback
- comp_state : comp_env_t
- comp_trigger_callback : _hal_comp_callback
- comp_trim : _efuse_trim1_t
- compid : ble_gap_peer_version_ind_t
- con_evt_cnt : ble_gap_conn_iq_report_t , ble_gap_evt_conn_iq_report_t
- con_interval : gap_conn_cmp_t
- con_intv_max : gap_slv_pref_t
- con_intv_min : gap_slv_pref_t
- con_latency : ble_gap_evt_subrate_chg_ind_t , ble_gap_subrate_chg_ind_t , gap_conn_cmp_t
- concentration : __attribute__
- conf : ble_sec_oob_t
- config_flag : esls_ap_sync_param_t
- conhdl : gap_conn_cmp_t
- conn_buf : stack_heaps_table_t
- conn_handle : ble_gap_evt_connected_t
- conn_idx : ags_evt_t , ams_c_evt_t , ancs_c_evt_t , ans_c_evt_t , ans_evt_t , bas_c_evt_t , bas_evt_t , bcs_evt_t , ble_gap_con_plan_tag_t , ccc_dk_c_evt_t , cscs_evt_t , cts_c_evt_t , cts_evt_t , dis_c_evt_t , dss_evt_t , esls_c_evt_t , esls_evt_t , gls_evt_t , gus_c_evt_t , gus_evt_t , hids_evt_t , hrrcps_evt_t , hrs_c_evt_t , hrs_evt_t , hts_evt_t , ias_c_evt_t , lls_c_evt_t , lms_evt_t , lns_evt_t , mlmr_c_evt_t , mlmr_evt_t , otas_c_evt_t , otas_evt_t , pass_c_evt_t , pass_evt_t , pcs_evt_t , ras_ad_evt_t , ras_c_ad_evt_t , ras_c_evt_t , rscs_c_evt_t , rscs_evt_t , rtus_evt_t , samples_evt_t , ths_c_evt_t , ths_evt_t , thscps_evt_t , thscps_rsp_val_t , tps_c_evt_t , uds_evt_t , wechat_evt_t , wss_evt_t
- conn_ind : ble_l2cap_evt_t
- conn_info : ble_gapc_evt_t
- conn_interval : ble_gap_evt_conn_param_updated_t , ble_gap_evt_connected_t
- conn_intv_max : ble_gap_ext_conn_param_t
- conn_intv_min : ble_gap_ext_conn_param_t
- conn_iq_report : ble_gapc_evt_t
- conn_latency : ble_gap_ext_conn_param_t
- conn_param_1m : ble_gap_ext_init_param_t
- conn_param_2m : ble_gap_ext_init_param_t
- conn_param_coded : ble_gap_ext_init_param_t
- conn_param_update_req : ble_gapc_evt_t
- conn_param_updated : ble_gapc_evt_t
- conn_req : ble_l2cap_evt_t
- conn_size : stack_heaps_table_t
- conn_timeout : ble_gap_init_param_t , gap_slv_pref_t
- conn_to : ble_gap_ext_init_param_t
- connected : ble_gapc_evt_t
- connless_iq_report : ble_gapc_evt_t
- consent_code : uds_evt_t
- ConstN : _ll_ecc_curve_init
- ConstP : _ll_ecc_curve_init , _pkc_montgomery_inversion , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- continuation_num : ble_gap_dft_subrate_param_t , ble_gap_subrate_req_t
- continuation_number : ble_gap_evt_subrate_chg_ind_t , ble_gap_subrate_chg_ind_t
- count : ble_gattc_char_desc_disc_t , ble_gattc_char_disc_t , ble_gattc_evt_char_desc_disc_t , ble_gattc_evt_char_disc_t , ble_gattc_evt_incl_disc_t , ble_gattc_evt_read_t , ble_gattc_evt_srvc_disc_t , ble_gattc_incl_disc_t , ble_gattc_read_rsp_t , ble_gattc_srvc_disc_t
- counter : _aon_wdt_init , _wdt_init
- counter_mode : _dual_timer_init , _ll_dual_timer_init
- counter_size : _ll_dual_timer_init
- cp_cmd_req_handler : cgms_init_t
- cp_code : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- cp_ret : cgms_cp_cmd_rsp_t
- cplt_attr_data : ams_c_evt_t
- crank_rev_data_present : cscs_meas_val_t
- crc32 : __attribute__
- crc_init : gdx_lcp_config_t
- credits : ble_l2cap_evt_sdu_recv_t , ble_l2cap_evt_sdu_send_t , ble_l2cap_lecb_add_credits_t , ble_l2cap_lecb_sdu_t , lecb_sdu_send_evt_t
- cs : app_dspi_pin_cfg_t , app_qspi_pin_cfg_t , app_spi_pin_cfg_t
- csn : app_graphics_dc_pins_t
- cte_count : gap_connless_cte_trans_param_t
- cte_len : gap_connless_cte_trans_param_t
- cte_req_interval : ble_gap_set_conn_cte_req_enable_t
- cte_req_len : ble_gap_set_conn_cte_req_enable_t
- cte_req_type : ble_gap_set_conn_cte_req_enable_t
- cte_type : ble_gap_conn_iq_report_t , ble_gap_connless_iq_report_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_connless_iq_report_t , ble_gap_per_sync_param_t , ble_gap_per_sync_trans_param_t , ble_gap_set_conn_cte_trans_param_t , gap_connless_cte_trans_param_t
- CTL_H : dma_block_config
- CTL_L : dma_block_config
- ctrl_pt_rsp : rscs_c_evt_t
- cts : app_uart_pin_cfg_t
- cts_cur_time_cccd_handle : cts_c_handles_t
- cts_cur_time_handle : cts_c_handles_t
- cts_loc_time_info_handle : cts_c_handles_t
- cts_ref_time_info_handle : cts_c_handles_t
- cts_srvc_end_handle : cts_c_handles_t
- cts_srvc_start_handle : cts_c_handles_t
- cumulative_crank_revs : cscs_meas_val_t
- cumulative_wheel_revs : cscs_meas_val_t
- cur_state : rtus_update_state_t
- cur_time : cts_c_evt_t , cts_evt_t , cts_init_t
- curr_path_loss : ble_gap_evt_path_loss_threshold_report_t , ble_gap_path_loss_threshold_report_t
- curr_tx_pwr_lvl : ble_gap_evt_local_tx_pwr_read_ind_t , ble_gap_local_tx_pwr_read_ind_t
- current_time_min : cts_updata_ref_time_info_t
- current_time_sec : cts_updata_ref_time_info_t