Macros
Clock Polarity
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_SCPOL_LOW 0x00000000UL
#define | LL_QSPI_SCPOL_HIGH (1UL << QSPI_CTRL0_SCPOL_Pos)
#define | LL_SPI_SCPOL_LOW 0x00000000UL
#define | LL_SPI_SCPOL_HIGH (1UL << SPI_CTRL0_SERIAL_CLK_POL_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_SCPOL_HIGH

#define LL_QSPI_SCPOL_HIGH (1UL << QSPI_CTRL0_SCPOL_Pos)

Clock to 1 when idle

Definition at line 474 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_SCPOL_LOW

#define LL_QSPI_SCPOL_LOW 0x00000000UL

Clock to 0 when idle

Definition at line 473 of file gr55xx_ll_qspi.h.

## ◆ LL_SPI_SCPOL_HIGH

#define LL_SPI_SCPOL_HIGH (1UL << SPI_CTRL0_SERIAL_CLK_POL_POS)

Clock to 1 when idle

Definition at line 276 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_SCPOL_LOW

#define LL_SPI_SCPOL_LOW 0x00000000UL

Clock to 0 when idle

Definition at line 275 of file gr55xx_ll_spi.h.