Macros
EXFLASH Size Information
Peripheral Driver » HAL Driver » EXFLASH » Defines » EXFLASH Exported Constants

## Macros
#define | EXFLASH_SIZE_PAGE_BYTES ((uint32_t)256)
#define | EXFLASH_SIZE_SECTOR_BYTES ((uint32_t)4096)
#define | EXFLASH_SIZE_CHIP_BYTES ((uint32_t)0x1000000)
#define | EXFLASH_START_ADDR FLASH_BASE
#define | EXFLASH_SIZE GR55XX_FLASH_SIZE
#define | EXFLASH_END_ADDR (EXFLASH_START_ADDR + EXFLASH_SIZE)
#define | EXFLASH_ALIAS_OFFSET (0x02000000UL)
#define | EXFLASH_ALIAS_ADDR (EXFLASH_START_ADDR + EXFLASH_ALIAS_OFFSET)

## Detailed Description

## Macro Definition Documentation

## ◆ EXFLASH_ALIAS_ADDR

#define EXFLASH_ALIAS_ADDR (EXFLASH_START_ADDR + EXFLASH_ALIAS_OFFSET)

Alias start address

Definition at line 231 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_ALIAS_OFFSET

#define EXFLASH_ALIAS_OFFSET (0x02000000UL)

Alias address offset

Definition at line 230 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_END_ADDR

#define EXFLASH_END_ADDR (EXFLASH_START_ADDR + EXFLASH_SIZE)

Flash end address

Definition at line 229 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE

#define EXFLASH_SIZE GR55XX_FLASH_SIZE

Flash size

Definition at line 228 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_CHIP_BYTES

#define EXFLASH_SIZE_CHIP_BYTES ((uint32_t)0x1000000)

Chip size in Bytes

Definition at line 226 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_PAGE_BYTES

#define EXFLASH_SIZE_PAGE_BYTES ((uint32_t)256)

Page size in Bytes

Definition at line 224 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_SIZE_SECTOR_BYTES

#define EXFLASH_SIZE_SECTOR_BYTES ((uint32_t)4096)

Sector size in Bytes

Definition at line 225 of file gr55xx_hal_exflash.h.

## ◆ EXFLASH_START_ADDR

#define EXFLASH_START_ADDR FLASH_BASE

Flash start address

Definition at line 227 of file gr55xx_hal_exflash.h.