### - r -

- RAS_AD_CP_MAX_LEN : ras_ad.h
- RAS_AD_DATA_MAX_LEN : ras_ad.h
- RAS_AD_DATA_OW_MAX_LEN : ras_ad.h
- RAS_AD_DATA_READY_MAX_LEN : ras_ad.h
- RAS_AD_FEA_MAX_LEN : ras_ad.h
- RAS_ANT_PATH_BIT_MASK : ras_common.h
- RAS_ANTENNA_PATH_1_MASK : ras_common.h
- RAS_ANTENNA_PATH_2_MASK : ras_common.h
- RAS_ANTENNA_PATH_3_MASK : ras_common.h
- RAS_ANTENNA_PATH_4_MASK : ras_common.h
- RAS_CACHE_PROC_NUM : ras.h
- RAS_CCCD_LEN : ras_common.h
- RAS_CFG_ID_BIT_MASK : ras_common.h
- RAS_CONNECTION_MAX : ras_common.h
- RAS_CTRL_PT_CHAR_MAX_LEN : ras_common.h
- RAS_CTRL_PT_OPCODE_LEN : ras_common.h
- RAS_CTRL_PT_OPCODE_OFFSET : ras_common.h
- RAS_CTRL_PT_OPERAND_MAX_LEN : ras_common.h
- RAS_CTRL_PT_OPERAND_OFFSET : ras_common.h
- RAS_ERROR_PROC_ALREADY_IN_PROGRESS : ras_common.h
- RAS_FEATURE_CHAR_LEN : ras_common.h
- RAS_LOG_INFO : ras_common.h
- RAS_MAX_PROC_NUM_PER_LINK : ras_common.h
- RAS_MODE0_DATA_BIT_MASK : ras_common.h
- RAS_MODE1_DATA_BIT_MASK : ras_common.h
- RAS_MODE2_DATA_BIT_MASK : ras_common.h
- RAS_MODE3_DATA_BIT_MASK : ras_common.h
- RAS_MODE_TYPE_BIT_MASK : ras_common.h
- RAS_MODE_TYPE_BIT_OFFSET : ras_common.h
- RAS_PCT_FORMAT_BIT_MASK : ras_common.h
- RAS_PCT_FORMAT_MASK : ras_common.h
- RAS_RANGING_COUNTER_BIT_MASK : ras_common.h
- RAS_RANGING_HEADER_LEN : ras_common.h
- RAS_ROLLING_SEGMENT_COUNTER_MAX : ras_common.h
- RAS_ROLLING_SEGMENT_COUNTER_MIN : ras_common.h
- RAS_SEGMENT_HEADER_FIRST_SEG_BITMASK : ras_common.h
- RAS_SEGMENT_HEADER_LAST_SEG_BITMASK : ras_common.h
- RAS_SEGMENT_HEADER_LEN : ras_common.h
- RAS_SEGMENT_HEADER_ROLL_SEG_COUNT_BITMASK : ras_common.h
- RAS_SUBEVENT_HEADER_FREQ_COMPENSATION_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_LEN : ras_common.h
- RAS_SUBEVENT_HEADER_NUM_STEPS_REPORTED_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_RANGING_DONE_STATUS_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_REF_POWER_LEVEL_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_START_ACL_CON_EVENT_OFFSET : ras_common.h
- RAS_SUBEVENT_HEADER_SUBEVENT_DONE_STATUS_OFFSET : ras_common.h
- READ_CFG0_CFG : gr55xx_ll_rtc.h
- RNG_LFSR_MODE_128BIT : gr55xx_hal_rng.h
- RNG_LFSR_MODE_59BIT : gr55xx_hal_rng.h
- RNG_OUTPUT_CYCLIC : gr55xx_hal_rng.h
- RNG_OUTPUT_CYCLIC_PARITY : gr55xx_hal_rng.h
- RNG_OUTPUT_FR0_S0 : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR_RNG : gr55xx_hal_rng.h
- RNG_POST_PRO_COUNTING : gr55xx_hal_rng.h
- RNG_POST_PRO_NEUMANN : gr55xx_hal_rng.h
- RNG_POST_PRO_NOT : gr55xx_hal_rng.h
- RNG_POST_PRO_SKIPPING : gr55xx_hal_rng.h
- RNG_SEED_FR0_S0 : gr55xx_hal_rng.h
- RNG_SEED_USER : gr55xx_hal_rng.h
- ROOT_PUBLIC_KEY_HASH_SIZE : gr55xx_efuse_layout.h
- RSA_U32_LENGTH : gr55xx_ll_pkc.h
- RSCS_C_CONNECTION_MAX : rscs_c.h
- RSCS_C_ERROR_CCCD_INVALID : rscs_c.h
- RSCS_C_ERROR_PROC_IN_PROGRESS : rscs_c.h
- RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT : rscs_c.h
- RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_FEAT_MULTIPLE_SENSORS_BIT : rscs_c.h
- RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs_c.h
- RSCS_C_FEAT_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_PT_RSP_LEN_MAX : rscs_c.h
- RSCS_CHAR_FULL : rscs.h
- RSCS_CHAR_MANDATORY : rscs.h
- RSCS_CHAR_SC_CTRL_POINT : rscs.h
- RSCS_CHAR_SENSOR_LOC_SUP : rscs.h
- RSCS_CONNECTION_MAX : rscs.h
- RSCS_CTRL_PT_RSP_LEN_MIN : rscs.h
- RSCS_CTRL_PT_VAL_LEN_MAX : rscs.h
- RSCS_ERROR_CCCD_INVALID : rscs.h
- RSCS_ERROR_PROC_IN_PROGRESS : rscs.h
- RSCS_FEAR_FULL_BIT : rscs.h
- RSCS_FEAT_CALIBRATION_PROCEDURE_BIT : rscs.h
- RSCS_FEAT_INSTANT_STRIDE_LEN_BIT : rscs.h
- RSCS_FEAT_MULTIPLE_SENSORS_BIT : rscs.h
- RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs.h
- RSCS_FEAT_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_FEAT_VAL_LEN_MAX : rscs.h
- RSCS_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs.h
- RSCS_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs.h
- RSCS_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_MEAS_VAL_LEN_MAX : rscs.h
- RSCS_SENSOR_LOC_VAL_LEN_MAX : rscs.h
- RTC_DIV_128 : gr55xx_hal_rtc.h
- RTC_DIV_16 : gr55xx_hal_rtc.h
- RTC_DIV_2 : gr55xx_hal_rtc.h
- RTC_DIV_32 : gr55xx_hal_rtc.h
- RTC_DIV_4 : gr55xx_hal_rtc.h
- RTC_DIV_64 : gr55xx_hal_rtc.h
- RTC_DIV_8 : gr55xx_hal_rtc.h
- RTC_DIV_NONE : gr55xx_hal_rtc.h
- RTC_FLAG_ALARM : gr55xx_hal_rtc.h
- RTC_FLAG_TICK : gr55xx_hal_rtc.h
- RTC_FLAG_WRAP : gr55xx_hal_rtc.h
- RTC_IT_ALARM : gr55xx_hal_rtc.h
- RTC_IT_TICK : gr55xx_hal_rtc.h
- RTC_IT_WRAP : gr55xx_hal_rtc.h
- RTUS_CHAR_FULL : rtus.h
- RTUS_CONNECTION_MAX : rtus.h
- RTUS_CTRL_PT_VAL_LEN : rtus.h
- RTUS_UPDATE_STATE_VAL_LEN : rtus.h