Macros
mode bits length for xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants

## Macros
#define | QSPI_CONCURRENT_XIP_MBL_2 LL_QSPI_CONCURRENT_XIP_MBL_2
#define | QSPI_CONCURRENT_XIP_MBL_4 LL_QSPI_CONCURRENT_XIP_MBL_4
#define | QSPI_CONCURRENT_XIP_MBL_8 LL_QSPI_CONCURRENT_XIP_MBL_8
#define | QSPI_CONCURRENT_XIP_MBL_16 LL_QSPI_CONCURRENT_XIP_MBL_16

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_MBL_16

#define QSPI_CONCURRENT_XIP_MBL_16 LL_QSPI_CONCURRENT_XIP_MBL_16

mode bits length equals to 16 bit.

Definition at line 580 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_MBL_2

#define QSPI_CONCURRENT_XIP_MBL_2 LL_QSPI_CONCURRENT_XIP_MBL_2

mode bits length equals to 2 bit.

Definition at line 577 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_MBL_4

#define QSPI_CONCURRENT_XIP_MBL_4 LL_QSPI_CONCURRENT_XIP_MBL_4

mode bits length equals to 4 bit.

Definition at line 578 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_MBL_8

#define QSPI_CONCURRENT_XIP_MBL_8 LL_QSPI_CONCURRENT_XIP_MBL_8

mode bits length equals to 8 bit.

Definition at line 579 of file gr55xx_hal_qspi.h.