Public Attributes | List of all members
dma_sg_llp_config Struct Reference
Peripheral Driver » HAL Driver » DMA » Structures » DMA Configuration

LL DMA sg and llp config definition. More...

`#include <gr55xx_hal_dma.h>`

## Public Attributes
dma_scatter_config_t | scatter_config
dma_gather_config_t | gather_config
dma_llp_config_t | llp_config

## Detailed Description

LL DMA sg and llp config definition.

Definition at line 218 of file gr55xx_hal_dma.h.

## Member Data Documentation

## ◆ gather_config

dma_gather_config_t dma_sg_llp_config::gather_config

Specifies the destination block chaining enable. This parameter can be a value DMA_LLP_DST_EN.

Definition at line 224 of file gr55xx_hal_dma.h.

## ◆ llp_config

dma_llp_config_t dma_sg_llp_config::llp_config

Specifies the linked list pointer. This parameter can be a value between 0x0 and 0xFFFFFFFF.(LLI accesses are always 32-bit accesses)

Definition at line 227 of file gr55xx_hal_dma.h.

## ◆ scatter_config

dma_scatter_config_t dma_sg_llp_config::scatter_config

Specifies the source block chaining enable. This parameter can be a value DMA_LLP_SRC_EN.

Definition at line 221 of file gr55xx_hal_dma.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_dma.h