Macros
Get Flags Defines
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

Flags definitions which can be used with LL_I2S_ReadReg function. More...

## Macros
#define | LL_I2S_STATUS_TXFO I2S_INT_STAT_TX_FIFO_OVER
#define | LL_I2S_STATUS_TXFE I2S_INT_STAT_TX_FIFO_EMPTY
#define | LL_I2S_STATUS_RXFO I2S_INT_STAT_RX_FIFO_OVER
#define | LL_I2S_STATUS_RXDA I2S_INT_STAT_RX_DATA_AVL

## Detailed Description

Flags definitions which can be used with LL_I2S_ReadReg function.

## Macro Definition Documentation

## ◆ LL_I2S_STATUS_RXDA

#define LL_I2S_STATUS_RXDA I2S_INT_STAT_RX_DATA_AVL

RX FIFO threshold level is reached flag

Definition at line 134 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_RXFO

#define LL_I2S_STATUS_RXFO I2S_INT_STAT_RX_FIFO_OVER

RX FIFO receive overflow flag

Definition at line 133 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_TXFE

#define LL_I2S_STATUS_TXFE I2S_INT_STAT_TX_FIFO_EMPTY

TX FIFO threshold level is not reached flag

Definition at line 132 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_STATUS_TXFO

#define LL_I2S_STATUS_TXFO I2S_INT_STAT_TX_FIFO_OVER

TX FIFO write overflow flag

Definition at line 131 of file gr55xx_ll_i2s.h.