### - l -

- LL_ADVS_DIS : gr55xx_ll_advs.h
- LL_ADVS_EN : gr55xx_ll_advs.h
- LL_ADVS_HIGHER_TYPE : gr55xx_ll_advs.h
- LL_ADVS_LIMIT_DIS : gr55xx_ll_advs.h
- LL_ADVS_LIMIT_EN : gr55xx_ll_advs.h
- LL_ADVS_LOWER_TYPE : gr55xx_ll_advs.h
- LL_AES_DMA_TRANSIZE_MAX : gr55xx_ll_aes.h
- LL_AES_DMA_TRANSIZE_MIN : gr55xx_ll_aes.h
- LL_AES_FLAG_DATAREADY : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_DONE : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_ERR : gr55xx_ll_aes.h
- LL_AES_FLAG_KEY_VALID : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_128 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_192 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_256 : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_AHB : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_KRAM : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_MCU : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_CBC : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_ECB : gr55xx_ll_aes.h
- LL_AES_ReadReg : gr55xx_ll_aes.h
- LL_AES_WriteReg : gr55xx_ll_aes.h
- LL_ANALOG_VOLTAGE_SCALE_DIS : gr55xx_ll_dvs.h
- LL_ANALOG_VOLTAGE_SCALE_EN : gr55xx_ll_dvs.h
- LL_ANALOG_VOLTAGE_SCALE_HIGHER_TYPE : gr55xx_ll_dvs.h
- LL_ANALOG_VOLTAGE_SCALE_LIMIT_DIS : gr55xx_ll_dvs.h
- LL_ANALOG_VOLTAGE_SCALE_LIMIT_EN : gr55xx_ll_dvs.h
- LL_ANALOG_VOLTAGE_SCALE_LOWER_TYPE : gr55xx_ll_dvs.h
- LL_AON_WD_TIMER_CLK_SEL_RNG : gr55xx_ll_aon_wdt.h
- LL_AON_WD_TIMER_CLK_SEL_RNG2 : gr55xx_ll_aon_wdt.h
- LL_AON_WD_TIMER_CLK_SEL_RTC : gr55xx_ll_aon_wdt.h
- LL_AON_WD_TIMER_CLK_SEL_XO : gr55xx_ll_aon_wdt.h
- LL_BOD2_DISABLE : gr55xx_ll_bod.h
- LL_BOD2_ENABLE : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_0 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_1 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_10 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_11 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_12 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_13 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_14 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_15 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_2 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_3 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_4 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_5 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_6 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_7 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_8 : gr55xx_ll_bod.h
- LL_BOD2_LEVEL_9 : gr55xx_ll_bod.h
- LL_BOD_DISABLE : gr55xx_ll_bod.h
- LL_BOD_ENABLE : gr55xx_ll_bod.h
- LL_BOD_STATIC_DISABLE : gr55xx_ll_bod.h
- LL_BOD_STATIC_ENABLE : gr55xx_ll_bod.h
- LL_CALENDAR_DIV_128 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_16 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_2 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_32 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_4 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_64 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_8 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_NONE : gr55xx_ll_calendar.h
- LL_CGC_FRC_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_DSPI_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C0_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C1_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C2_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C3_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_S_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_PDM_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_PWM_0_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_PWM_1_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI0_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI1_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI2_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIALS_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPI_M_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPI_S_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART0_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART1_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART2_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART3_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_VTTBL_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_AES_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_HMAC_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_PKC_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_PRESENT_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_RAMKEY_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_MISC_CLK : gr55xx_ll_cgc.h
- LL_CGC_MCU_MISC_CLK_DEFAULT : gr55xx_ll_cgc.h
- LL_CGC_MCU_MISC_DMA_CLK : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_DEFAULT : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_LP_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF : gr55xx_ll_cgc.h
- LL_CGC_MCU_PERIPH_SLP_CG_DEFAULT : gr55xx_ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_ALL : gr55xx_ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_HCLK : gr55xx_ll_cgc.h
- LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_AES_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_HMAC_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_PKC_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_PRESENT_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_RAMKEY_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN : gr55xx_ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_CLK0 : gr55xx_ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK0 : gr55xx_ll_cgc.h
- LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK1 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_WFI_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CLDR_TIMER_CLK_SEL_RNG : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_CLK_SEL_RNG2 : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_CLK_SEL_RTC : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_CLK_SEL_XO : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_TICK : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_TICK_TYPE_AUTO : gr55xx_ll_calendar.h
- LL_CLDR_TIMER_TICK_TYPE_SINGLE : gr55xx_ll_calendar.h
- LL_CLK_AON_CLK_WAKUP_CLK_DIS : gr55xx_ll_clk.h
- LL_CLK_AON_CLK_WAKUP_CLK_EN : gr55xx_ll_clk.h
- LL_CLK_CAL_CLK_SOURCE_RNG_32K : gr55xx_ll_clk_cal.h
- LL_CLK_CAL_CLK_SOURCE_RNG_40K : gr55xx_ll_clk_cal.h
- LL_CLK_CAL_CLK_SOURCE_RTC_32K : gr55xx_ll_clk_cal.h
- LL_CLK_CPLL_F48M_CLK : gr55xx_ll_clk.h
- LL_CLK_CPLL_S16M_CLK : gr55xx_ll_clk.h
- LL_CLK_CPLL_S64M_CLK : gr55xx_ll_clk.h
- LL_CLK_CPLL_S96M_CLK : gr55xx_ll_clk.h
- LL_CLK_CPLL_T24M_CLK : gr55xx_ll_clk.h
- LL_CLK_CPLL_T32M_CLK : gr55xx_ll_clk.h
- LL_CLK_SEL_FAST_WAKEUP_CPLL_CLK : gr55xx_ll_clk.h
- LL_CLK_SEL_FAST_WAKEUP_HF_OSC_CLK : gr55xx_ll_clk.h
- LL_CLK_SEL_SOURCE_CPLL_CLK : gr55xx_ll_clk.h
- LL_CLK_SEL_SOURCE_HF_OSC_CLK : gr55xx_ll_clk.h
- LL_CLK_XO_PLL_HF_STAT : gr55xx_ll_clk.h
- LL_CLK_XO_PLL_PLL_STAT : gr55xx_ll_clk.h
- LL_CLK_XO_PLL_XO_STAT : gr55xx_ll_clk.h
- LL_CLK_XO_S16M_CLK : gr55xx_ll_clk.h
- LL_CONC_QSPI_DEFAULT_CONFIG : gr55xx_ll_qspi.h
- LL_DDVS_AUTO_MODE : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_DIS : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_EN : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_SEL_SYS_16M : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_SEL_SYS_32M : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_SEL_XO_16M : gr55xx_ll_ddvs.h
- LL_DDVS_CLK_SEL_XO_32M : gr55xx_ll_ddvs.h
- LL_DDVS_DIS : gr55xx_ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_16K : gr55xx_ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_4K : gr55xx_ll_ddvs.h
- LL_DDVS_DIVIDE_FACTOR_8K : gr55xx_ll_ddvs.h
- LL_DDVS_EN : gr55xx_ll_ddvs.h
- LL_DDVS_MALNUAL_MODE : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_0_EN : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_1_EN : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_2_EN : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_3_EN : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_ALL_DIS : gr55xx_ll_ddvs.h
- LL_DDVS_RINGO_ALL_EN : gr55xx_ll_ddvs.h
- LL_DMA0_PERIPH_I2C2_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C2_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C3_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C3_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C4_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C4_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C5_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_I2C5_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_MEM : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_OSPI_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_OSPI_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_QSPI0_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_QSPI0_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_QSPI1_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_QSPI1_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_SNSADC : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_SPIM_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_SPIM_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_SPIS_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_SPIS_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART0_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART0_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART1_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART1_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART2_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART2_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART3_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART3_TX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART4_RX : gr55xx_ll_dma.h
- LL_DMA0_PERIPH_UART4_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_DSPIM_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_DSPIM_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2C0_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2C0_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2C1_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2C1_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2S_M_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2S_M_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2S_S_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_I2S_S_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_MEM : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_OSPI_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_OSPI_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_PDM_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI1_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI1_RX_2 : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI1_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI1_TX_2 : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI2_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_QSPI2_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_SPIM_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_SPIM_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART0_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART0_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART3_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART3_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART4_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART4_TX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART5_RX : gr55xx_ll_dma.h
- LL_DMA1_PERIPH_UART5_TX : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_0 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_1 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_2 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_3 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_4 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_5 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_6 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_7 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_ALL : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_WORD : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_PERIPH : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_PERIPH : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_DST_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_NO_CHANGE : gr55xx_ll_dma.h
- LL_DMA_DST_SCATTER_DISABLE : gr55xx_ll_dma.h
- LL_DMA_DST_SCATTER_ENABLE : gr55xx_ll_dma.h
- LL_DMA_DST_STAT_UPDATE_DISABLE : gr55xx_ll_dma.h
- LL_DMA_DST_STAT_UPDATE_ENABLE : gr55xx_ll_dma.h
- LL_DMA_LLP_DST_DISABLE : gr55xx_ll_dma.h
- LL_DMA_LLP_DST_ENABLE : gr55xx_ll_dma.h
- LL_DMA_LLP_SRC_DISABLE : gr55xx_ll_dma.h
- LL_DMA_LLP_SRC_ENABLE : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_ALL_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_DST_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_SRC_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_SINGLE_BLOCK : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_0 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_1 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_2 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_3 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_4 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_5 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_6 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_7 : gr55xx_ll_dma.h
- LL_DMA_ReadReg : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_WORD : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_SRC_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_GATHER_DISABLE : gr55xx_ll_dma.h
- LL_DMA_SRC_GATHER_ENABLE : gr55xx_ll_dma.h
- LL_DMA_SRC_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_NO_CHANGE : gr55xx_ll_dma.h
- LL_DMA_SRC_STAT_UPDATE_DISABLE : gr55xx_ll_dma.h
- LL_DMA_SRC_STAT_UPDATE_ENABLE : gr55xx_ll_dma.h
- LL_DMA_WriteReg : gr55xx_ll_dma.h
- LL_DUAL_TIMER_COUNTERSIZE_16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_COUNTERSIZE_32 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_FREERUNNING_MODE : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PERIODIC_MODE : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV0 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV256 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_ReadReg : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_WriteReg : gr55xx_ll_dual_tim.h
- LL_ECC_CURVE_DEFAULT_CONFIG : gr55xx_ll_pkc.h
- LL_ECC_CURVE_SECP256K1_CONFIG : gr55xx_ll_pkc.h
- LL_ECC_CURVE_SECP256R1_CONFIG : gr55xx_ll_pkc.h
- LL_EFUSE_CRC_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_SUCCESS : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_SUCCESS : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_DIS_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_EN_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_ReadReg : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_READ : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM_BUSY : gr55xx_ll_efuse.h
- LL_EFUSE_WriteReg : gr55xx_ll_efuse.h
- LL_GPIO_DEFAULT_CONFIG : gr55xx_ll_gpio.h
- LL_GPIO_INPUT_TYPE_CMOS : gr55xx_ll_gpio.h
- LL_GPIO_INPUT_TYPE_SCHMITT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_INOUT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_INPUT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_INPUT_POS : gr55xx_ll_gpio.h
- LL_GPIO_MODE_NONE : gr55xx_ll_gpio.h
- LL_GPIO_MODE_OUTPUT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_OUTPUT_POS : gr55xx_ll_gpio.h
- LL_GPIO_MUX_0 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_1 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_2 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_3 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_4 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_5 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_6 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_7 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_0 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_1 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_10 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_11 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_12 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_13 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_14 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_15 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_2 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_3 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_4 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_5 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_6 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_7 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_9 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_ALL : gr55xx_ll_gpio.h
- LL_GPIO_PULL_DOWN : gr55xx_ll_gpio.h
- LL_GPIO_PULL_NO : gr55xx_ll_gpio.h
- LL_GPIO_PULL_UP : gr55xx_ll_gpio.h
- LL_GPIO_ReadReg : gr55xx_ll_gpio.h
- LL_GPIO_SPEED_HIGH : gr55xx_ll_gpio.h
- LL_GPIO_SPEED_MEDIUM : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_DS0_MASK : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_DS0_POS : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_DS1_MASK : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_DS1_POS : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_HIGH : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_LOW : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_MEDIUM : gr55xx_ll_gpio.h
- LL_GPIO_STRENGTH_ULTRA : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_BOTH_EDGE : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_FALLING : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_HIGH : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_LOW : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_NONE : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_RISING : gr55xx_ll_gpio.h
- LL_GPIO_WriteReg : gr55xx_ll_gpio.h
- LL_HMAC_CALCULATETYPE_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_CALCULATETYPE_SHA : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MAX : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MIN : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_SHA : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_DONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_ERR : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_MESSAGEDONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_KEY_VALID : gr55xx_ll_hmac.h
- LL_HMAC_HASH_STANDARD : gr55xx_ll_hmac.h
- LL_HMAC_HASH_USER : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_AHB : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_KRAM : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_MCU : gr55xx_ll_hmac.h
- LL_HMAC_ReadReg : gr55xx_ll_hmac.h
- LL_HMAC_WriteReg : gr55xx_ll_hmac.h
- LL_I2C_ABRT_10ADDR1_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10ADDR2_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10B_RD_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_7B_ADDR_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_ARB_LOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_READ : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_MST_DIS : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SDA_STUCK_AT_LOW : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLV_ARBLOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVFLUSH_TXFIFO : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVRD_INTX : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TX_FLUSH_CNT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TXDATA_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_USER_ABRT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_10BIT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_7BIT : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_RESTART : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_STOP : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_READ : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_WRITE : gr55xx_ll_i2c.h
- LL_I2C_CMD_SLV_NONE : gr55xx_ll_i2c.h
- LL_I2C_DEFAULT_CONFIG : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_SCL_STUCK_AT_LOW : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_SCL_STUCK_AT_LOW : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_OVER : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_10BIT : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_7BIT : gr55xx_ll_i2c.h
- LL_I2C_ReadReg : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_10 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_11 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_12 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_13 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_14 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_15 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_16 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_17 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_18 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_19 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_20 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_21 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_22 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_23 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_24 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_25 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_26 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_27 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_28 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_29 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_30 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_31 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_32 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_8 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_9 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_FULL : gr55xx_ll_i2c.h
- LL_I2C_SPEED_1000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_100K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_2000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_400K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_FAST : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_HIGH : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_STANDARD : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_10 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_11 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_12 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_13 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_14 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_15 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_16 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_17 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_18 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_19 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_20 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_21 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_22 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_23 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_24 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_25 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_26 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_27 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_28 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_29 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_30 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_31 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_32 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_8 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_9 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_WriteReg : gr55xx_ll_i2c.h
- LL_I2S_APB_WIDTH_16BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_32BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_8BIT : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_1 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_2 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_3 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_4 : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_32M : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_64M : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_96M : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_12BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_16BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_20BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_24BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_32BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_IGNORE : gr55xx_ll_i2s.h
- LL_I2S_DEFAULT_CONFIG : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_16 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_2 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_4 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_8 : gr55xx_ll_i2s.h
- LL_I2S_FULL_DUPLEX : gr55xx_ll_i2s.h
- LL_I2S_INT_RXDA : gr55xx_ll_i2s.h
- LL_I2S_INT_RXFO : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFE : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFO : gr55xx_ll_i2s.h
- LL_I2S_ReadReg : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_12BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_16BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_20BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_24BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_32BIT : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_12 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_20 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_NONE : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_RX : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_TX : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXDA : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXFO : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFE : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_10FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_11FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_12FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_13FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_14FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_15FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_16FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_1FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_2FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_3FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_4FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_5FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_6FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_7FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_8FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_9FIFO : gr55xx_ll_i2s.h
- LL_I2S_WriteReg : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_32 : gr55xx_ll_i2s.h
- LL_ISO7816_ACTION_NONE : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_ON : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_STOPCLK : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TXRX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_WARMRST : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_ABSENT : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_PRESENT : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_HIGH : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_LOW : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_DEFAULT : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_INVERSE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DMA_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DONE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_MASK_ALL : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_PRESENCE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RETRY_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RX_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_STATE_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_TEST : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX_WAIT : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX_GUARD : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS0 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS1 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_POST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_PRE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ReadReg : gr55xx_ll_iso7816.h
- LL_ISO7816_WriteReg : gr55xx_ll_iso7816.h
- LL_PKC_BIGMULTI_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MIN : gr55xx_ll_pkc.h
- LL_PKC_INTEN_BAOVF : gr55xx_ll_pkc.h
- LL_PKC_INTEN_DONE : gr55xx_ll_pkc.h
- LL_PKC_INTEN_ERR : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_ADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERMULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_COMPARE : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_INVERTION : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_LEFTSHIFT : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_MULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_SUB : gr55xx_ll_pkc.h
- LL_PKC_ReadReg : gr55xx_ll_pkc.h
- LL_PKC_WORKSTAT_BUSY : gr55xx_ll_pkc.h
- LL_PKC_WriteReg : gr55xx_ll_pkc.h
- LL_PWM_ACTIONEVENT_CLEAR : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_NONE : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_SET : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_TOGGLE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_MODE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_CENTER_ALIGNED : gr55xx_ll_pwm.h
- LL_PWM_CHANNEL_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- LL_PWM_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_NEGATIVE : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_POSITIVE : gr55xx_ll_pwm.h
- LL_PWM_EDGE_ALIGNED : gr55xx_ll_pwm.h
- LL_PWM_FLICKER_MODE : gr55xx_ll_pwm.h
- LL_PWM_HOLD_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_ReadReg : gr55xx_ll_pwm.h
- LL_PWM_STOP_LVL_HIGH : gr55xx_ll_pwm.h
- LL_PWM_STOP_LVL_LOW : gr55xx_ll_pwm.h
- LL_PWM_WriteReg : gr55xx_ll_pwm.h
- LL_QSPI0_REG_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI0_REG_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI0_XIP_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI0_XIP_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI1_REG_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI1_REG_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI1_XIP_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI1_XIP_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI2_REG_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI2_REG_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI2_XIP_RX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI2_XIP_TX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_0BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_12BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_20BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_24BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_28BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_32BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_36BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_40BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_44BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_48BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_52BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_56BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_60BIT : gr55xx_ll_qspi.h
- LL_QSPI_ADDRSIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_CLK_STRETCH_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CLK_STRETCH_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_CONT_XFER_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_CONT_XFER_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_DFS_BYTE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_DFS_HARDCODE_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_DFS_HARDCODE_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_DFS_WORD : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_FRF_RSVD : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INSTSIZE_0BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INSTSIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INSTSIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_INSTSIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MBL_16 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MBL_2 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MBL_4 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MBL_8 : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MODE_BITS_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_MODE_BITS_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_PREFETCH_DISABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_PREFETCH_ENABLE : gr55xx_ll_qspi.h
- LL_QSPI_CONCURRENT_XIP_SLAVE0 : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_10BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_11BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_12BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_13BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_14BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_15BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_17BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_18BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_19BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_20BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_21BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_22BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_23BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_24BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_25BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_26BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_27BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_28BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_29BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_30BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_31BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_32BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_5BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_6BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_7BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_DATASIZE_9BIT : gr55xx_ll_qspi.h
- LL_QSPI_DEFAULT_CONFIG : gr55xx_ll_qspi.h
- LL_QSPI_DMA_RX_DIS : gr55xx_ll_qspi.h
- LL_QSPI_DMA_RX_EN : gr55xx_ll_qspi.h
- LL_QSPI_DMA_TX_DIS : gr55xx_ll_qspi.h
- LL_QSPI_DMA_TX_EN : gr55xx_ll_qspi.h
- LL_QSPI_FRF_DUALSPI : gr55xx_ll_qspi.h
- LL_QSPI_FRF_QUADSPI : gr55xx_ll_qspi.h
- LL_QSPI_FRF_SPI : gr55xx_ll_qspi.h
- LL_QSPI_FULL_DUPLEX : gr55xx_ll_qspi.h
- LL_QSPI_IM_ALL : gr55xx_ll_qspi.h
- LL_QSPI_IM_MST : gr55xx_ll_qspi.h
- LL_QSPI_IM_RXF : gr55xx_ll_qspi.h
- LL_QSPI_IM_RXO : gr55xx_ll_qspi.h
- LL_QSPI_IM_RXU : gr55xx_ll_qspi.h
- LL_QSPI_IM_SPITE : gr55xx_ll_qspi.h
- LL_QSPI_IM_TXE : gr55xx_ll_qspi.h
- LL_QSPI_IM_TXO : gr55xx_ll_qspi.h
- LL_QSPI_IM_TXU : gr55xx_ll_qspi.h
- LL_QSPI_IM_XRXO : gr55xx_ll_qspi.h
- LL_QSPI_INST_ADDR_ALL_IN_SPI : gr55xx_ll_qspi.h
- LL_QSPI_INST_ADDR_ALL_IN_SPIFRF : gr55xx_ll_qspi.h
- LL_QSPI_INST_IN_SPI_ADDR_IN_SPIFRF : gr55xx_ll_qspi.h
- LL_QSPI_INSTSIZE_0BIT : gr55xx_ll_qspi.h
- LL_QSPI_INSTSIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_INSTSIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_INSTSIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_IS_ALL : gr55xx_ll_qspi.h
- LL_QSPI_IS_MST : gr55xx_ll_qspi.h
- LL_QSPI_IS_RXF : gr55xx_ll_qspi.h
- LL_QSPI_IS_RXO : gr55xx_ll_qspi.h
- LL_QSPI_IS_RXU : gr55xx_ll_qspi.h
- LL_QSPI_IS_SPITE : gr55xx_ll_qspi.h
- LL_QSPI_IS_TXE : gr55xx_ll_qspi.h
- LL_QSPI_IS_TXO : gr55xx_ll_qspi.h
- LL_QSPI_IS_TXU : gr55xx_ll_qspi.h
- LL_QSPI_IS_XRXO : gr55xx_ll_qspi.h
- LL_QSPI_MAX_FIFO_DEPTH : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_HANDSHAKE_DIS : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_HANDSHAKE_EN : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_NON_SEQUENTIAL : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_RX : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_SEQUENTIAL : gr55xx_ll_qspi.h
- LL_QSPI_MICROWIRE_TX : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_10BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_11BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_12BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_13BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_14BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_15BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_16BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_1BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_2BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_3BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_4BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_5BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_6BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_7BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_8BIT : gr55xx_ll_qspi.h
- LL_QSPI_MW_CMDSIZE_9BIT : gr55xx_ll_qspi.h
- LL_QSPI_NORMAL_MODE : gr55xx_ll_qspi.h
- LL_QSPI_PROTOCOL_MICROWIRE : gr55xx_ll_qspi.h
- LL_QSPI_PROTOCOL_MOTOROLA : gr55xx_ll_qspi.h
- LL_QSPI_PROTOCOL_TI : gr55xx_ll_qspi.h
- LL_QSPI_READ_EEPROM : gr55xx_ll_qspi.h
- LL_QSPI_RIS_ALL : gr55xx_ll_qspi.h
- LL_QSPI_RIS_MST : gr55xx_ll_qspi.h
- LL_QSPI_RIS_RXF : gr55xx_ll_qspi.h
- LL_QSPI_RIS_RXO : gr55xx_ll_qspi.h
- LL_QSPI_RIS_RXU : gr55xx_ll_qspi.h
- LL_QSPI_RIS_SPITE : gr55xx_ll_qspi.h
- LL_QSPI_RIS_TXE : gr55xx_ll_qspi.h
- LL_QSPI_RIS_TXO : gr55xx_ll_qspi.h
- LL_QSPI_RIS_TXU : gr55xx_ll_qspi.h
- LL_QSPI_RIS_XRXO : gr55xx_ll_qspi.h
- LL_QSPI_RX_SAMPLE_NEGATIVE_EDGE : gr55xx_ll_qspi.h
- LL_QSPI_RX_SAMPLE_POSITIVE_EDGE : gr55xx_ll_qspi.h
- LL_QSPI_SCPHA_1EDGE : gr55xx_ll_qspi.h
- LL_QSPI_SCPHA_2EDGE : gr55xx_ll_qspi.h
- LL_QSPI_SCPOL_HIGH : gr55xx_ll_qspi.h
- LL_QSPI_SCPOL_LOW : gr55xx_ll_qspi.h
- ll_qspi_set_xfer_size : gr55xx_ll_qspi.h
- LL_QSPI_SIMPLEX_RX : gr55xx_ll_qspi.h
- LL_QSPI_SIMPLEX_TX : gr55xx_ll_qspi.h
- LL_QSPI_SLAVE0 : gr55xx_ll_qspi.h
- LL_QSPI_SLAVE1 : gr55xx_ll_qspi.h
- LL_QSPI_SLAVE_OUTDIS : gr55xx_ll_qspi.h
- LL_QSPI_SLAVE_OUTEN : gr55xx_ll_qspi.h
- LL_QSPI_SR_BUSY : gr55xx_ll_qspi.h
- LL_QSPI_SR_DCOL : gr55xx_ll_qspi.h
- LL_QSPI_SR_RFF : gr55xx_ll_qspi.h
- LL_QSPI_SR_RFNE : gr55xx_ll_qspi.h
- LL_QSPI_SR_TFE : gr55xx_ll_qspi.h
- LL_QSPI_SR_TFNF : gr55xx_ll_qspi.h
- LL_QSPI_SR_TXE : gr55xx_ll_qspi.h
- LL_QSPI_TEST_MODE : gr55xx_ll_qspi.h
- LL_RNG_IT_DISABLE : gr55xx_ll_rng.h
- LL_RNG_IT_ENABLE : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_128BIT : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_59BIT : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC_PARITY : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR_RNG : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_COUNTING : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NEUMANN : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NOT : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_SKIPPING : gr55xx_ll_rng.h
- LL_RNG_ReadReg : gr55xx_ll_rng.h
- LL_RNG_SEED_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_SEED_USER : gr55xx_ll_rng.h
- LL_RNG_WriteReg : gr55xx_ll_rng.h
- LL_RTC_DIV_128 : gr55xx_ll_rtc.h
- LL_RTC_DIV_16 : gr55xx_ll_rtc.h
- LL_RTC_DIV_2 : gr55xx_ll_rtc.h
- LL_RTC_DIV_32 : gr55xx_ll_rtc.h
- LL_RTC_DIV_4 : gr55xx_ll_rtc.h
- LL_RTC_DIV_64 : gr55xx_ll_rtc.h
- LL_RTC_DIV_8 : gr55xx_ll_rtc.h
- LL_RTC_DIV_NONE : gr55xx_ll_rtc.h
- LL_RTC_TIMER_CLK_SEL_RNG : gr55xx_ll_rtc.h
- LL_RTC_TIMER_CLK_SEL_RNG2 : gr55xx_ll_rtc.h
- LL_RTC_TIMER_CLK_SEL_RTC : gr55xx_ll_rtc.h
- LL_RTC_TIMER_CLK_SEL_XO : gr55xx_ll_rtc.h
- LL_RTC_TIMER_TICK_TYPE_AUTO : gr55xx_ll_rtc.h
- LL_RTC_TIMER_TICK_TYPE_SINGLE : gr55xx_ll_rtc.h
- LL_SPI_DATASIZE_10BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_11BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_12BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_13BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_14BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_15BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_16BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_17BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_18BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_19BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_20BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_21BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_22BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_23BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_24BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_25BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_26BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_27BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_28BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_29BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_30BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_31BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_32BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_4BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_5BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_6BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_7BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_8BIT : gr55xx_ll_spi.h
- LL_SPI_DATASIZE_9BIT : gr55xx_ll_spi.h
- LL_SPI_DMA_RX_DIS : gr55xx_ll_spi.h
- LL_SPI_DMA_RX_EN : gr55xx_ll_spi.h
- LL_SPI_DMA_TX_DIS : gr55xx_ll_spi.h
- LL_SPI_DMA_TX_EN : gr55xx_ll_spi.h
- LL_SPI_FULL_DUPLEX : gr55xx_ll_spi.h
- LL_SPI_IM_MST : gr55xx_ll_spi.h
- LL_SPI_IM_RXF : gr55xx_ll_spi.h
- LL_SPI_IM_RXO : gr55xx_ll_spi.h
- LL_SPI_IM_RXU : gr55xx_ll_spi.h
- LL_SPI_IM_TXE : gr55xx_ll_spi.h
- LL_SPI_IM_TXO : gr55xx_ll_spi.h
- LL_SPI_IS_MST : gr55xx_ll_spi.h
- LL_SPI_IS_RXF : gr55xx_ll_spi.h
- LL_SPI_IS_RXO : gr55xx_ll_spi.h
- LL_SPI_IS_RXU : gr55xx_ll_spi.h
- LL_SPI_IS_TXE : gr55xx_ll_spi.h
- LL_SPI_IS_TXO : gr55xx_ll_spi.h
- LL_SPI_M_FIFO_DEPTH : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_HANDSHAKE_DIS : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_HANDSHAKE_EN : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_NON_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_RX : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SPI_MICROWIRE_TX : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_10BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_11BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_12BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_13BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_14BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_15BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_16BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_1BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_2BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_3BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_4BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_5BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_6BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_7BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_8BIT : gr55xx_ll_spi.h
- LL_SPI_MW_CMDSIZE_9BIT : gr55xx_ll_spi.h
- LL_SPI_NORMAL_MODE : gr55xx_ll_spi.h
- LL_SPI_PROTOCOL_MICROWIRE : gr55xx_ll_spi.h
- LL_SPI_PROTOCOL_MOTOROLA : gr55xx_ll_spi.h
- LL_SPI_PROTOCOL_TI : gr55xx_ll_spi.h
- LL_SPI_READ_EEPROM : gr55xx_ll_spi.h
- LL_SPI_ReadReg : gr55xx_ll_spi.h , gr55xx_ll_qspi.h
- LL_SPI_RIS_MST : gr55xx_ll_spi.h
- LL_SPI_RIS_RXF : gr55xx_ll_spi.h
- LL_SPI_RIS_RXO : gr55xx_ll_spi.h
- LL_SPI_RIS_RXU : gr55xx_ll_spi.h
- LL_SPI_RIS_TXE : gr55xx_ll_spi.h
- LL_SPI_RIS_TXO : gr55xx_ll_spi.h
- LL_SPI_S_FIFO_DEPTH : gr55xx_ll_spi.h
- LL_SPI_SCPHA_1EDGE : gr55xx_ll_spi.h
- LL_SPI_SCPHA_2EDGE : gr55xx_ll_spi.h
- LL_SPI_SCPOL_HIGH : gr55xx_ll_spi.h
- LL_SPI_SCPOL_LOW : gr55xx_ll_spi.h
- LL_SPI_SIMPLEX_RX : gr55xx_ll_spi.h
- LL_SPI_SIMPLEX_TX : gr55xx_ll_spi.h
- LL_SPI_SLAVE0 : gr55xx_ll_spi.h
- LL_SPI_SLAVE1 : gr55xx_ll_spi.h
- LL_SPI_SLAVE_OUTDIS : gr55xx_ll_spi.h
- LL_SPI_SLAVE_OUTEN : gr55xx_ll_spi.h
- LL_SPI_SR_BUSY : gr55xx_ll_spi.h
- LL_SPI_SR_DCOL : gr55xx_ll_spi.h
- LL_SPI_SR_RFF : gr55xx_ll_spi.h
- LL_SPI_SR_RFNE : gr55xx_ll_spi.h
- LL_SPI_SR_TFE : gr55xx_ll_spi.h
- LL_SPI_SR_TFNF : gr55xx_ll_spi.h
- LL_SPI_SR_TXE : gr55xx_ll_spi.h
- LL_SPI_TEST_MODE : gr55xx_ll_spi.h
- LL_SPI_WriteReg : gr55xx_ll_qspi.h , gr55xx_ll_spi.h
- LL_SPIM_DEFAULT_CONFIG : gr55xx_ll_spi.h
- LL_SPIS_DEFAULT_CONFIG : gr55xx_ll_spi.h
- LL_TIMER_ReadReg : gr55xx_ll_tim.h
- LL_TIMER_WriteReg : gr55xx_ll_tim.h
- LL_UART_CTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_CTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_DATABITS_5B : gr55xx_ll_uart.h
- LL_UART_DATABITS_6B : gr55xx_ll_uart.h
- LL_UART_DATABITS_7B : gr55xx_ll_uart.h
- LL_UART_DATABITS_8B : gr55xx_ll_uart.h
- LL_UART_DEFAULT_CONFIG : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_NONE : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_RTS_CTS : gr55xx_ll_uart.h
- LL_UART_IER_MS : gr55xx_ll_uart.h
- LL_UART_IER_RDA : gr55xx_ll_uart.h
- LL_UART_IER_RLS : gr55xx_ll_uart.h
- LL_UART_IER_THRE : gr55xx_ll_uart.h
- LL_UART_IIR_CTO : gr55xx_ll_uart.h
- LL_UART_IIR_MS : gr55xx_ll_uart.h
- LL_UART_IIR_NIP : gr55xx_ll_uart.h
- LL_UART_IIR_RDA : gr55xx_ll_uart.h
- LL_UART_IIR_RLS : gr55xx_ll_uart.h
- LL_UART_IIR_THRE : gr55xx_ll_uart.h
- LL_UART_LSR_BI : gr55xx_ll_uart.h
- LL_UART_LSR_FE : gr55xx_ll_uart.h
- LL_UART_LSR_OE : gr55xx_ll_uart.h
- LL_UART_LSR_PE : gr55xx_ll_uart.h
- LL_UART_LSR_RFE : gr55xx_ll_uart.h
- LL_UART_LSR_TEMT : gr55xx_ll_uart.h
- LL_UART_LSR_THRE : gr55xx_ll_uart.h
- LL_UART_PARITY_EVEN : gr55xx_ll_uart.h
- LL_UART_PARITY_NONE : gr55xx_ll_uart.h
- LL_UART_PARITY_ODD : gr55xx_ll_uart.h
- LL_UART_PARITY_SP0 : gr55xx_ll_uart.h
- LL_UART_PARITY_SP1 : gr55xx_ll_uart.h
- LL_UART_ReadReg : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_CHAR_1 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_FULL_2 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1_5 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_2 : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_CHAR_2 : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_EMPTY : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- LL_UART_USR_RFF : gr55xx_ll_uart.h
- LL_UART_USR_RFNE : gr55xx_ll_uart.h
- LL_UART_USR_TFE : gr55xx_ll_uart.h
- LL_UART_USR_TFNF : gr55xx_ll_uart.h
- LL_UART_WriteReg : gr55xx_ll_uart.h
- LL_WDT_LOCK_WR_ACCESS_DISABLE : gr55xx_ll_wdt.h
- LL_WDT_LOCK_WR_ACCESS_ENABLE : gr55xx_ll_wdt.h
- LL_WDT_ReadReg : gr55xx_ll_wdt.h
- LL_WDT_WriteReg : gr55xx_ll_wdt.h
- LL_XQSPI_1ST_PREFETCH_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_1ST_PREFETCH_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_16M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_24M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_32M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_48M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_64M : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_DIRECT_MAP_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_DIRECT_MAP_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_NORMAL : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FLUSH_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FLUSH_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_NORMAL : gr55xx_ll_xqspi.h
- LL_XQSPI_DEFAULT_CONFIG : gr55xx_ll_xqspi.h
- LL_XQSPI_DISABLE_PRESENT : gr55xx_ll_xqspi.h
- LL_XQSPI_ENABLE_PRESENT : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_128BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_32BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_HP_MODE_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_HP_MODE_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_QSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_XIP : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_12BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_16BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_20BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_24BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_28BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_32BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_4BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_8BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_DEPTH : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_2 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_8 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_3_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_DUALSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_QUADSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_SPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_LSB : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_MSB : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_BUSY : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_ReadReg : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_1EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_2EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_HIGH : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_LOW : gr55xx_ll_xqspi.h
- LL_XQSPI_WriteReg : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_3BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_4BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_FAST_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_BIG : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_LITTLE : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS0 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS1 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS2 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS3 : gr55xx_ll_xqspi.h
- LLS_C_CONNECTION_MAX : lls_c.h
- LMS_CONNECTION_MAX : lms.h
- LMS_MAX_DATA_LEN : lms.h
- LMS_PATTERN_VALUE : lms.h
- LMS_SERVICE_UUID : lms.h
- LNS_CONNECTION_MAX : lns.h
- LNS_LOG_CTRL_PT_VAL_LEN : lns.h
- LNS_LOG_INFO_VAL_LEN : lns.h
- LNS_SERVICE_UUID : lns.h
- LOCAL_INT_DISABLE : gr55xx_hal.h
- LOCAL_INT_RESTORE : gr55xx_hal.h