Macros
: endian mode for qspi xip
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0 0u /* Default endian order from AHB */
#define | LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1 1u /* Re-order the read data as [23:16], [31:24], [7:0], [15:8] */
#define | LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2 2u /* Re-order the read data as [7:0], [15:8], [23:16], [31:24] */

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0

#define LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0 0u /* Default endian order from AHB */

Definition at line 564 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1

#define LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1 1u /* Re-order the read data as [23:16], [31:24], [7:0], [15:8] */

Definition at line 565 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2

#define LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2 2u /* Re-order the read data as [7:0], [15:8], [23:16], [31:24] */

Definition at line 566 of file gr55xx_ll_qspi.h.