Macros
Block2 Clock During WFI
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK
#define | LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK
#define | LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_WFI_ALL_HCLK2

#define LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)

All clock group 2

Definition at line 105 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_SECU_DIV4_PCLK

#define LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK

Div4 clk for security blocks

Definition at line 102 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_XQSPI_DIV4_PCLK

#define LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK

Div4 clk for xf qspi

Definition at line 103 of file gr55xx_ll_cgc.h.