Public Attributes | List of all members
cgms_racp_rsp_t Struct Reference
BLE Services » Continuous Continuous Glucose Monitoring Monitoring Service Record Access Control Point (CGMS_RACP) » Structures

Continuous Glucose Monitoring Recoerd Access Control Point response value. More...

`#include <cgms_racp.h>`

## Public Attributes
cgms_racp_op_code_t | op_code
cgms_racp_operator_t | operator
union {
uint16_t num_of_record
struct {
cgms_racp_op_code_t op_code
cgms_racp_operand_t status
} rsp
} | operand

## Detailed Description

Continuous Glucose Monitoring Recoerd Access Control Point response value.

Definition at line 143 of file cgms_racp.h.

## Member Data Documentation

## ◆ num_of_record

uint16_t cgms_racp_rsp_t::num_of_record

Number of record (if op_code = CGMS_RACP_OP_REP_NB_OF_STRD_RECS).

Definition at line 149 of file cgms_racp.h.

## ◆ op_code

cgms_racp_op_code_t cgms_racp_rsp_t::op_code

Continuous Glucose Monitoring Recoerd Access Control Point Operation Code.

Request Op Code.

Definition at line 145 of file cgms_racp.h.

## ◆ operand

union { ... } cgms_racp_rsp_t::operand

Response operand.

## ◆ operator

cgms_racp_operator_t cgms_racp_rsp_t::operator

Continuous Glucose Monitoring Recoerd Access Control Point Operator.

Definition at line 146 of file cgms_racp.h.

## ◆ rsp

struct { ... } cgms_racp_rsp_t::rsp

Response.

## ◆ status

cgms_racp_operand_t cgms_racp_rsp_t::status

Command Status (if op_code = CGMS_RACP_OP_RSP_CODE).

Definition at line 153 of file cgms_racp.h.

The documentation for this struct was generated from the following file:

- cgms_racp.h