Public Attributes | List of all members
ble_gap_get_bd_addr_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Get broadcast address struct. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | index
ble_gap_bdaddr_t | bd_addr

## Detailed Description

Get broadcast address struct.

Definition at line 326 of file ble_gapc.h.

## Member Data Documentation

## ◆ bd_addr

ble_gap_bdaddr_t ble_gap_get_bd_addr_t::bd_addr

BD address.

Definition at line 329 of file ble_gapc.h.

## ◆ index

uint8_t ble_gap_get_bd_addr_t::index

Advertsing index. The valid range is: 0 - 4.

Definition at line 328 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h