Macros
SPI Flags Definition
Peripheral Driver » HAL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | SPI_FLAG_DCOL LL_SPI_SR_DCOL
#define | SPI_FLAG_TXE LL_SPI_SR_TXE
#define | SPI_FLAG_RFF LL_SPI_SR_RFF
#define | SPI_FLAG_RFNE LL_SPI_SR_RFNE
#define | SPI_FLAG_TFE LL_SPI_SR_TFE
#define | SPI_FLAG_TFNF LL_SPI_SR_TFNF
#define | SPI_FLAG_BUSY LL_SPI_SR_BUSY

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_FLAG_BUSY

#define SPI_FLAG_BUSY LL_SPI_SR_BUSY

Busy flag

Definition at line 390 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_DCOL

#define SPI_FLAG_DCOL LL_SPI_SR_DCOL

Data collision error flag

Definition at line 384 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_RFF

#define SPI_FLAG_RFF LL_SPI_SR_RFF

Rx FIFO full flag

Definition at line 386 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_RFNE

#define SPI_FLAG_RFNE LL_SPI_SR_RFNE

Rx FIFO not empty flag

Definition at line 387 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_TFE

#define SPI_FLAG_TFE LL_SPI_SR_TFE

Tx FIFO empty flag

Definition at line 388 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_TFNF

#define SPI_FLAG_TFNF LL_SPI_SR_TFNF

Tx FIFO not full flag

Definition at line 389 of file gr55xx_hal_spi.h.

## ◆ SPI_FLAG_TXE

#define SPI_FLAG_TXE LL_SPI_SR_TXE

Transmission error flag

Definition at line 385 of file gr55xx_hal_spi.h.