Macros
: address size for concurrent xip mode
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT 0x0
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT 0x1
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT 0x2
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT 0x3
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT 0x4
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT 0x5
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT 0x6
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT 0x7
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT 0x8
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT 0x9
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT 0xA
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT 0xB
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT 0xC
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT 0xD
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT 0xE
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT 0xF

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT 0x0

Address length for QSPI XIP transfer: 0 bits

Definition at line 604 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT 0x3

Address length for QSPI XIP transfer: 12 bits

Definition at line 607 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT 0x4

Address length for QSPI XIP transfer: 16 bits

Definition at line 608 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT 0x5

Address length for QSPI XIP transfer: 20 bits

Definition at line 609 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT 0x6

Address length for QSPI XIP transfer: 24 bits

Definition at line 610 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT 0x7

Address length for QSPI XIP transfer: 28 bits

Definition at line 611 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT 0x8

Address length for QSPI XIP transfer: 32 bits

Definition at line 612 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT 0x9

Address length for QSPI XIP transfer: 36 bits

Definition at line 613 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT 0xA

Address length for QSPI XIP transfer: 40 bits

Definition at line 614 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT 0xB

Address length for QSPI XIP transfer: 44 bits

Definition at line 615 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT 0xC

Address length for QSPI XIP transfer: 48 bits

Definition at line 616 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT 0x1

Address length for QSPI XIP transfer: 4 bits

Definition at line 605 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT 0xD

Address length for QSPI XIP transfer: 52 bits

Definition at line 617 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT 0xE

Address length for QSPI XIP transfer: 56 bits

Definition at line 618 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT 0xF

Address length for QSPI XIP transfer: 60 bits

Definition at line 619 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT 0x2

Address length for QSPI XIP transfer: 8 bits

Definition at line 606 of file gr55xx_ll_qspi.h.