Public Attributes | List of all members
app_graphics_dc_cmd_t Struct Reference
Peripheral Driver » APP DRIVER » DC » Structures

Define Control Command for DC Frame. More...

`#include <app_graphics_dc.h>`

## Public Attributes
uint8_t | command
uint32_t | address
app_graphics_dc_frame_address_width_e | address_width
app_graphics_dc_frame_timing_e | frame_timing

## Detailed Description

Define Control Command for DC Frame.

Definition at line 294 of file app_graphics_dc.h.

## Member Data Documentation

## ◆ address

uint32_t app_graphics_dc_cmd_t::address

Address phase for display timing,if no address phase, ignore this

Definition at line 296 of file app_graphics_dc.h.

## ◆ address_width

app_graphics_dc_frame_address_width_e app_graphics_dc_cmd_t::address_width

Optional values: GDC_FRAME_ADDRESS_WIDTH_NONE GDC_FRAME_ADDRESS_WIDTH_08BIT GDC_FRAME_ADDRESS_WIDTH_16BIT GDC_FRAME_ADDRESS_WIDTH_24BIT

Definition at line 297 of file app_graphics_dc.h.

## ◆ command

uint8_t app_graphics_dc_cmd_t::command

Command phase for display timing

Definition at line 295 of file app_graphics_dc.h.

## ◆ frame_timing

app_graphics_dc_frame_timing_e app_graphics_dc_cmd_t::frame_timing

Specify the supported frame timing

Definition at line 301 of file app_graphics_dc.h.

The documentation for this struct was generated from the following file:

- app_graphics_dc.h