Macros
InitStrcut default configuration
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Exported Constants

## Macros
#define | LL_GPIO_DEFAULT_CONFIG
| LL GPIO InitStrcut default configuration. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_DEFAULT_CONFIG

#define LL_GPIO_DEFAULT_CONFIG

Value:
{ \
.pin = LL_GPIO_PIN_ALL, \
.mode = LL_GPIO_MODE_INPUT, \
.pull = LL_GPIO_PULL_DOWN, \
.mux = LL_GPIO_MUX_8, \
.speed = LL_GPIO_SPEED_MEDIUM, \
.strength = LL_GPIO_STRENGTH_MEDIUM, \
.input_type = LL_GPIO_INPUT_TYPE_CMOS, \
.trigger = LL_GPIO_TRIGGER_NONE, \
}

LL GPIO InitStrcut default configuration.

Definition at line 281 of file gr55xx_ll_gpio.h.

LL_GPIO_SPEED_MEDIUM
#define LL_GPIO_SPEED_MEDIUM
Definition: gr55xx_ll_gpio.h:200
LL_GPIO_MUX_8
#define LL_GPIO_MUX_8
Definition: gr55xx_ll_gpio.h:194
LL_GPIO_TRIGGER_NONE
#define LL_GPIO_TRIGGER_NONE
Definition: gr55xx_ll_gpio.h:223
LL_GPIO_PULL_DOWN
#define LL_GPIO_PULL_DOWN
Definition: gr55xx_ll_gpio.h:180
LL_GPIO_MODE_INPUT
#define LL_GPIO_MODE_INPUT
Definition: gr55xx_ll_gpio.h:170
LL_GPIO_STRENGTH_MEDIUM
#define LL_GPIO_STRENGTH_MEDIUM
Definition: gr55xx_ll_gpio.h:208
LL_GPIO_PIN_ALL
#define LL_GPIO_PIN_ALL
Definition: gr55xx_ll_gpio.h:163
LL_GPIO_INPUT_TYPE_CMOS
#define LL_GPIO_INPUT_TYPE_CMOS
Definition: gr55xx_ll_gpio.h:216