Macros
RX/TX resolution of one channel
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_RESOLUTION_12BIT (0UL)
#define | LL_I2S_RESOLUTION_16BIT (1UL)
#define | LL_I2S_RESOLUTION_20BIT (2UL)
#define | LL_I2S_RESOLUTION_24BIT (3UL)
#define | LL_I2S_RESOLUTION_32BIT (4UL)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_RESOLUTION_12BIT

#define LL_I2S_RESOLUTION_12BIT (0UL)

12 bits resolution.

Definition at line 216 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_RESOLUTION_16BIT

#define LL_I2S_RESOLUTION_16BIT (1UL)

16 bits resolution.

Definition at line 217 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_RESOLUTION_20BIT

#define LL_I2S_RESOLUTION_20BIT (2UL)

20 bits resolution.

Definition at line 218 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_RESOLUTION_24BIT

#define LL_I2S_RESOLUTION_24BIT (3UL)

24 bits resolution.

Definition at line 219 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_RESOLUTION_32BIT

#define LL_I2S_RESOLUTION_32BIT (4UL)

32 bits resolution.

Definition at line 220 of file gr55xx_ll_i2s.h.