Macros
XQSPI Clock Speed
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_BAUD_RATE_64M LL_XQSPI_BAUD_RATE_64M
#define | XQSPI_BAUD_RATE_48M LL_XQSPI_BAUD_RATE_48M
#define | XQSPI_BAUD_RATE_32M LL_XQSPI_BAUD_RATE_32M
#define | XQSPI_BAUD_RATE_24M LL_XQSPI_BAUD_RATE_24M
#define | XQSPI_BAUD_RATE_16M LL_XQSPI_BAUD_RATE_16M

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_BAUD_RATE_16M

#define XQSPI_BAUD_RATE_16M LL_XQSPI_BAUD_RATE_16M

Serial clock speed is 16 MHz

Definition at line 313 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_24M

#define XQSPI_BAUD_RATE_24M LL_XQSPI_BAUD_RATE_24M

Serial clock speed is 24 MHz

Definition at line 312 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_32M

#define XQSPI_BAUD_RATE_32M LL_XQSPI_BAUD_RATE_32M

Serial clock speed is 32 MHz

Definition at line 311 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_48M

#define XQSPI_BAUD_RATE_48M LL_XQSPI_BAUD_RATE_48M

Serial clock speed is 48 MHz

Definition at line 310 of file gr55xx_hal_xqspi.h.

## ◆ XQSPI_BAUD_RATE_64M

#define XQSPI_BAUD_RATE_64M LL_XQSPI_BAUD_RATE_64M

Serial clock speed is 64 MHz

Definition at line 309 of file gr55xx_hal_xqspi.h.