Here is a list of all file members with links to the files they belong to:

### - o -

- OE_SET : gr55xx_ll_gpio.h
- offset_ext_1p0 : gr55xx_efuse_layout.h
- offset_int_0p8 : gr55xx_efuse_layout.h
- offset_int_1p2 : gr55xx_efuse_layout.h
- offset_int_1p6 : gr55xx_efuse_layout.h
- ONE_TIME : gr55xx_hal_rtc.h
- OPEN_RAS_LOG : ras_common.h
- OPENED : gr55xx_hal_rtc.h
- OSPI_ACCESS_MEMORY : app_graphics_ospi.h
- OSPI_ACCESS_REGISTER : app_graphics_ospi.h
- OSPI_ACCESS_UNSET : app_graphics_ospi.h
- OSPI_CLOCK_FREQ_16MHz : app_graphics_ospi.h
- OSPI_CLOCK_FREQ_24MHz : app_graphics_ospi.h
- OSPI_CLOCK_FREQ_32MHz : app_graphics_ospi.h
- OSPI_CLOCK_FREQ_48MHz : app_graphics_ospi.h
- ospi_irq_handler : app_graphics_ospi.h
- OSPI_PASR_BOTTOM_1MB : app_graphics_ospi.h
- OSPI_PASR_BOTTOM_2MB : app_graphics_ospi.h
- OSPI_PASR_BOTTOM_4MB : app_graphics_ospi.h
- OSPI_PASR_FULL : app_graphics_ospi.h
- OSPI_PASR_MAX : app_graphics_ospi.h
- OSPI_PASR_NONE : app_graphics_ospi.h
- OSPI_PASR_TOP_1MB : app_graphics_ospi.h
- OSPI_PASR_TOP_2MB : app_graphics_ospi.h
- OSPI_PASR_TOP_4MB : app_graphics_ospi.h
- OSPI_PHY_DELAY_TAP_2 : app_graphics_ospi.h
- OSPI_PHY_DELAY_TAP_3 : app_graphics_ospi.h
- OSPI_PHY_DELAY_TAP_4 : app_graphics_ospi.h
- OSPI_PSRAM_BYTE_SIZE : app_graphics_ospi.h
- OSPI_PSRAM_DEVICE_ID : app_graphics_ospi.h
- OSPI_PSRAM_DRV_STR_FULL : app_graphics_ospi.h
- OSPI_PSRAM_DRV_STR_HALF : app_graphics_ospi.h
- OSPI_PSRAM_DRV_STR_ONE_EIGHTH : app_graphics_ospi.h
- OSPI_PSRAM_DRV_STR_ONE_FORTH : app_graphics_ospi.h
- OSPI_PSRAM_MAX_XIP_ADDRESS : app_graphics_ospi.h
- OSPI_PSRAM_MIN_XIP_ADDRESS : app_graphics_ospi.h
- OSPI_PSRAM_RD_LATENCY_3 : app_graphics_ospi.h
- OSPI_PSRAM_RD_LATENCY_4 : app_graphics_ospi.h
- OSPI_PSRAM_RD_LATENCY_5 : app_graphics_ospi.h
- OSPI_PSRAM_RD_LATENCY_6 : app_graphics_ospi.h
- OSPI_PSRAM_RD_LATENCY_7 : app_graphics_ospi.h
- OSPI_PSRAM_WR_LATENCY_3 : app_graphics_ospi.h
- OSPI_PSRAM_WR_LATENCY_4 : app_graphics_ospi.h
- OSPI_PSRAM_WR_LATENCY_5 : app_graphics_ospi.h
- OSPI_PSRAM_WR_LATENCY_6 : app_graphics_ospi.h
- OSPI_PSRAM_WR_LATENCY_7 : app_graphics_ospi.h
- OSPI_STATE_ACTIVE : app_graphics_ospi.h
- OSPI_STATE_DEEP_SLEEP : app_graphics_ospi.h
- OSPI_STATE_HALF_SLEEP : app_graphics_ospi.h
- OTAS_C_CONNECTION_MAX : otas_c.h
- otas_c_ctrl_data_send() : otas_c.h
- OTAS_C_CTRL_PT_OP_DFU_ENTER : otas_c.h
- otas_c_disc_srvc_start() : otas_c.h
- OTAS_C_EVT_CTRL_SUCCESS : otas_c.h
- OTAS_C_EVT_DISCOVERY_COMPLETE : otas_c.h
- OTAS_C_EVT_DISCOVERY_FAIL : otas_c.h
- otas_c_evt_handler_t : otas_c.h
- OTAS_C_EVT_INVALID : otas_c.h
- OTAS_C_EVT_PEER_DATA_RECEIVE : otas_c.h
- OTAS_C_EVT_TX_CPLT : otas_c.h
- OTAS_C_EVT_TX_NTF_SET_SUCCESS : otas_c.h
- otas_c_evt_type_t : otas_c.h
- OTAS_C_EVT_WRITE_OP_ERR : otas_c.h
- otas_c_tx_data_send() : otas_c.h
- otas_c_tx_notify_set() : otas_c.h
- otas_client_init() : otas_c.h
- OTAS_CONNECTION_MAX : otas.h
- OTAS_CTRL_CHAR_UUID : otas_c.h
- otas_ctrl_pt_op_code_t : otas.h
- OTAS_CTRL_PT_OP_DFU_ENTER : otas.h
- OTAS_CTRL_PT_OP_RESERVED : otas.h
- OTAS_CTRL_PT_OP_RSP_CODE : otas.h
- OTAS_DFU_MODE_COPY_UPGRADE : otas.h
- OTAS_DFU_MODE_NON_COPY_UPGRADE : otas.h
- OTAS_DFU_MODE_RESERVED : otas.h
- otas_dfu_mode_t : otas.h
- OTAS_EVT_CTRL_PT_INDICATION_DISABLED : otas.h
- OTAS_EVT_CTRL_PT_INDICATION_ENABLED : otas.h
- OTAS_EVT_DFU_MODE_SET : otas.h
- OTAS_EVT_DFU_TASK_ENTER : otas.h
- OTAS_EVT_DISCONNECT : otas.h
- otas_evt_handler_t : otas.h
- OTAS_EVT_INVALID : otas.h
- OTAS_EVT_NOTIFY_COMPLETE : otas.h
- OTAS_EVT_RX_RECEIVE_DATA : otas.h
- OTAS_EVT_TX_NOTIFICATION_DISABLED : otas.h
- OTAS_EVT_TX_NOTIFICATION_ENABLED : otas.h
- otas_evt_type_t : otas.h
- OTAS_MAX_DATA_LEN : otas.h
- otas_notify_tx_data() : otas.h
- OTAS_RX_CHAR_UUID : otas_c.h
- otas_service_init() : otas.h
- otas_service_start_handle_get() : otas.h
- OTAS_SVC_UUID : otas_c.h
- OTAS_TX_CHAR_UUID : otas_c.h
- OTAS_VERSION : otas.h
- overflow_det_t : gr55xx_hal_rtc.h