Public Attributes | List of all members
ble_gap_set_path_loss_report_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Set path loss reporting parameter info. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | high_thr
uint8_t | high_hyst
uint8_t | low_thr
uint8_t | low_hyst
uint16_t | min_conn_evt_num

## Detailed Description

Set path loss reporting parameter info.

Definition at line 730 of file ble_gapc.h.

## Member Data Documentation

## ◆ high_hyst

uint8_t ble_gap_set_path_loss_report_param_t::high_hyst

Hysteresis value for the high threshold (dB).

Definition at line 733 of file ble_gapc.h.

## ◆ high_thr

uint8_t ble_gap_set_path_loss_report_param_t::high_thr

High threshold for the path loss (dB).

Definition at line 732 of file ble_gapc.h.

## ◆ low_hyst

uint8_t ble_gap_set_path_loss_report_param_t::low_hyst

Hysteresis value for the low threshold (dB).

Definition at line 735 of file ble_gapc.h.

## ◆ low_thr

uint8_t ble_gap_set_path_loss_report_param_t::low_thr

Low threshold for the path loss (dB).

Definition at line 734 of file ble_gapc.h.

## ◆ min_conn_evt_num

uint16_t ble_gap_set_path_loss_report_param_t::min_conn_evt_num

Minimum time in number of connection events to be observed.

Definition at line 736 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h