Macros
Clock Phase
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_SCPHA_1EDGE 0x00000000UL
#define | LL_QSPI_SCPHA_2EDGE (1UL << QSPI_CTRL0_SCPHA_Pos)
#define | LL_SPI_SCPHA_1EDGE 0x00000000UL
#define | LL_SPI_SCPHA_2EDGE (1UL << SPI_CTRL0_SERIAL_CLK_PHASE_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_SCPHA_1EDGE

#define LL_QSPI_SCPHA_1EDGE 0x00000000UL

First clock transition is the first data capture edge

Definition at line 466 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_SCPHA_2EDGE

#define LL_QSPI_SCPHA_2EDGE (1UL << QSPI_CTRL0_SCPHA_Pos)

Second clock transition is the first data capture edge

Definition at line 467 of file gr55xx_ll_qspi.h.

## ◆ LL_SPI_SCPHA_1EDGE

#define LL_SPI_SCPHA_1EDGE 0x00000000UL

First clock transition is the first data capture edge

Definition at line 268 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_SCPHA_2EDGE

#define LL_SPI_SCPHA_2EDGE (1UL << SPI_CTRL0_SERIAL_CLK_PHASE_POS)

Second clock transition is the first data capture edge

Definition at line 269 of file gr55xx_ll_spi.h.