Macros
: transfer of inst & address for concurrent xip mode
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI 0x0
#define | LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF 0x1
#define | LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF 0x2

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI

#define LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI 0x0

Instruction and address are sent in SPI mode

Definition at line 625 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF

#define LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF 0x2

Instruction and address are sent in Daul/Quad SPI mode

Definition at line 627 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF

#define LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF 0x1

Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode

Definition at line 626 of file gr55xx_ll_qspi.h.