Macros
Action state.
Peripheral Driver » LL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | LL_ISO7816_ACTION_NONE 0x00000000U
#define | LL_ISO7816_ACTION_OFF 0x00000001U
#define | LL_ISO7816_ACTION_STOPCLK 0x00000002U
#define | LL_ISO7816_ACTION_ON 0x00000003U
#define | LL_ISO7816_ACTION_WARMRST 0x00000004U
#define | LL_ISO7816_ACTION_RX 0x00000005U
#define | LL_ISO7816_ACTION_TX 0x00000006U
#define | LL_ISO7816_ACTION_TXRX 0x00000007U

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ISO7816_ACTION_NONE

#define LL_ISO7816_ACTION_NONE 0x00000000U

Do Nothing.

Definition at line 100 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_OFF

#define LL_ISO7816_ACTION_OFF 0x00000001U

Switch Off.

Definition at line 101 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_ON

#define LL_ISO7816_ACTION_ON 0x00000003U

Switch on and receive ATR.

Definition at line 103 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_RX

#define LL_ISO7816_ACTION_RX 0x00000005U

Receive.

Definition at line 105 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_STOPCLK

#define LL_ISO7816_ACTION_STOPCLK 0x00000002U

Stop the clock.

Definition at line 102 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_TX

#define LL_ISO7816_ACTION_TX 0x00000006U

Transmit.

Definition at line 106 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_TXRX

#define LL_ISO7816_ACTION_TXRX 0x00000007U

Transmit, followed by RX.

Definition at line 107 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_ACTION_WARMRST

#define LL_ISO7816_ACTION_WARMRST 0x00000004U

Trigger warm reset and receive ATR.

Definition at line 104 of file gr55xx_ll_iso7816.h.