Here is a list of all class members with links to the classes they belong to:

### - m -

- main_ctrl_section : __attribute__
- main_key_section : __attribute__
- major : sdk_version_t
- mantissa : bps_ieee_float16_t , gls_ieee_float16_t , ieee_float32_t
- manuf_name : ble_gap_dev_version_ind_t
- manufact_name_str : dis_init_t
- manufacturer_id : dis_c_sys_id_t , dis_sys_id_t
- map : ble_gap_chnl_map_t
- master_ack_count : _i2c_handle
- max : cgms_racp_req_t , gls_racp_filter_t
- max_adv_data_len : ble_gap_dev_info_t
- max_adv_evt : ble_gap_adv_time_param_t
- max_cte_len : ble_gap_antenna_inf_t
- max_data_len : ble_gap_dev_info_t
- max_image_idx : esls_char_infor_t
- max_latency : ble_gap_dft_subrate_param_t , ble_gap_subrate_req_t
- max_meas_interval_sup : hts_init_t
- max_nb_attr : ble_gatts_create_db_t
- max_rx_octets : ble_gap_evt_data_length_t , ble_gap_le_pkt_size_ind_t
- max_rx_time : ble_gap_evt_data_length_t , ble_gap_le_pkt_size_ind_t
- max_size : ble_gatts_attm_desc_128_t , ble_gatts_attm_desc_t
- max_skip : ble_gap_adv_second_cfg_t
- max_smaple_cte : ble_gap_connless_iq_sample_param_t
- max_switching_pattern_len : ble_gap_antenna_inf_t
- max_tx_octets : ble_gap_evt_data_length_t , ble_gap_le_pkt_size_ind_t
- max_tx_pwr : ble_gap_adv_param_t , ble_gap_dev_tx_power_t , ble_gap_ext_adv_param_t
- max_tx_pwr_lvl : ble_gap_evt_local_tx_pwr_read_ind_t , ble_gap_local_tx_pwr_read_ind_t
- max_tx_time : ble_gap_evt_data_length_t , ble_gap_le_pkt_size_ind_t
- meal : gls_meas_ctx_t
- mean_arterial_pr : bps_meas_t
- meas_ctx : gls_rec_t
- meas_interval : hts_init_t
- meas_loc : __attribute__ , cgms_init_t
- meas_status : bps_meas_t
- meas_status_present : bps_meas_t
- meas_type : __attribute__ , cgms_init_t
- meas_val : gls_rec_t
- medication : gls_meas_ctx_t
- medication_id : gls_meas_ctx_t
- memory_power_size : __attribute__
- min : __attribute__ , _calendar_alarm , _calendar_time , cgms_racp_req_t , gls_racp_filter_t , prf_date_time_t
- min_conn_evt_num : ble_gap_set_path_loss_report_param_t
- min_meas_interval_sup : hts_init_t
- min_tx_pwr : ble_gap_dev_tx_power_t
- minor : sdk_version_t
- mipicfg_format : app_graphics_dc_params_t
- miso : app_dspi_pin_cfg_t , app_spi_pin_cfg_t
- mks_flag : ble_gap_lepsm_register_t
- mlmr_c_flow_ctrl_cccd_handle : mlmr_c_handles_t
- mlmr_c_flow_ctrl_handle : mlmr_c_handles_t
- mlmr_c_rx_handle : mlmr_c_handles_t
- mlmr_c_srvc_end_handle : mlmr_c_handles_t
- mlmr_c_srvc_start_handle : mlmr_c_handles_t
- mlmr_c_tx_cccd_handle : mlmr_c_handles_t
- mlmr_c_tx_handle : mlmr_c_handles_t
- mmap_key : _qspi_memorymapped_set_t
- mmap_val : _qspi_memorymapped_set_t
- mode : _aon_gpio_init , _calendar_handle , _dma_init , _gpio_init , _hmac_init , _i2c_handle , _ll_dma_init , _ll_gpio_init , _ll_pwm_init_t , _ll_xqspi_init_t , _msio_init , _tick_handle_t , app_gpiote_param_t , app_io_init_t , app_qspi_pin_t , app_spi_pin_t , ble_gap_per_sync_trans_param_t , gdx_lcp_config_t , pwm_init_t , ras_filter_data_operand_t
- model_num_str : dis_init_t
- mon : _calendar_time
- month : __attribute__ , birth_date_t , prf_date_time_t
- mosi : app_dspi_pin_cfg_t , app_spi_pin_cfg_t
- mps : ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t
- ms : _calendar_time
- msg_ret : stack_heaps_table_t
- msg_ret_size : stack_heaps_table_t
- msio_callback : _hal_msio_callback
- msp_deinit : _hal_callback
- msp_init : _hal_callback
- mspi_mode : app_graphics_dc_params_t
- mtu : ble_gatt_common_evt_mtu_exchange_t , ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t , thscps_test_conn_info_t
- mtu_exchange : ble_gatt_common_evt_t
- multi_channel : adc_env_t
- multi_ntf : ble_gatts_evt_t
- multi_user_present : wss_init_t
- muscle_mass : bcs_meas_val_t
- muscle_mass_present : bcs_meas_flag_t
- muscle_percentage : bcs_meas_val_t
- muscle_percentage_present : bcs_meas_flag_t
- mux : _aon_gpio_init , _gpio_init , _ll_gpio_init , _msio_init , app_adc_pin_t , app_comp_pin_t , app_dspi_pin_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_pdm_pin_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t