Here is a list of all class members with links to the classes they belong to:

### - r -

- racp_filter_type : gls_racp_filter_t
- racp_operator : gls_racp_filter_t , gls_racp_rsp_t
- racp_req_handler : cgms_init_t
- ram_size : _efuse_trim0_t
- rand : ble_sec_oob_t
- random_data : app_rng_evt_t
- random_func : pkc_init_t
- random_number : _rng_handle
- ranging_cmp_ind : ble_gapc_evt_t
- ranging_ind : ble_gapc_evt_t
- ranging_sample_report : ble_gapc_evt_t
- ranging_status : ble_gap_evt_ranging_cmp_ind_t , ble_gap_evt_ranging_ind_t
- ras_counter : ras_ctr_data_operand_t , ras_ctr_lost_data_seg_operand_t
- ras_features : ras_c_read_rsp_t
- ras_num : ras_cmp_data_rsp_operand_t
- rate_of_dec_alert_level : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- rate_of_inc_alert_level : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- rd : _ll_qspi_memorymapped_init_t
- rd_lc : app_graphics_ospi_params_t
- read_cmd : _ll_xqspi_init_t , _xqspi_init_t
- read_fifo : _i2s_handle , _qspi_handle , _spi_handle
- read_ntf_ind_rsp : ras_c_ad_evt_t
- read_req : ble_gatts_evt_t
- read_rsp : ble_gattc_evt_t , dis_c_evt_t , ras_c_evt_t
- read_spsm_rsp : ccc_dk_c_evt_t
- read_type : ras_c_read_rsp_t
- read_write_fifo : _spi_handle
- reason : ble_gap_evt_adv_stop_t , ble_gap_evt_disconnected_t , ble_gap_evt_scan_stop_t , ble_gap_evt_tx_pwr_change_report_t , ble_gap_tx_pwr_change_report_t , ble_l2cap_evt_disconnect_t , ble_sec_evt_key_missing_t , lecb_disconn_ind_t
- rec_data_buffer : dfu_buffer_t
- rec_data_buffer_size : dfu_buffer_t
- rec_delete_func : cgms_init_t
- rec_get_func : cgms_init_t
- rec_num_get_func : cgms_init_t
- received_length : ags_stream_env_t
- red : esls_c_led_infor_t
- ref : hids_report_int_t
- ref_time_info : cts_adj_info_t , cts_c_evt_t , cts_init_t
- reg_cert_data_list : dis_init_t
- regi_user_name_present : uds_regi_user_data_flag_t
- remote_tx_pwr_read : ble_gapc_evt_t
- report_disable : ble_gap_per_sync_param_t
- report_flag : ble_gap_sync_established_ind_t
- report_id : hids_report_ref_t
- report_map : hids_init_t
- report_type : hids_evt_t , hids_report_ref_t
- req_type : ble_sec_cfm_enc_t , ble_sec_enc_req_t , ble_sec_evt_enc_req_t
- reserved : __attribute__ , _efuse_trim1_t , ags_header_first_ext_t , ags_header_first_t , dfu_boot_info_t , uds_regi_user_data_flag_t
- reserved0 : _efuse_trim0_t
- reserved1 : _efuse_trim0_t
- reserved2 : _efuse_trim0_t
- reserved3 : _efuse_trim0_t
- reserved_1 : ags_ack_packet_t
- reserved_2 : ags_ack_packet_t
- reset_mode : _wdt_init
- resolution_x : app_graphics_dc_framelayer_t , app_graphics_dc_params_t
- resolution_y : app_graphics_dc_framelayer_t , app_graphics_dc_params_t
- result_code : ags_ack_packet_t
- retention : _adc_handle , _aes_handle , _comp_handle , _dma_handle , _dspi_handle , _gpadc_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pdm_handle , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _uart_handle , pwm_handle_t
- retr_ra_data_param : ras_ctr_pt_operation_t
- retry : _exflash_handle , _xqspi_handle_t
- right_rate : thscps_test_info_t
- ringer_set : pass_c_evt_t
- ringer_setting : pass_init_t
- rkey_dist : ble_sec_param_t
- rng_env : app_rng_params_t
- rng_msp_deinit : _hal_rng_callback
- rng_msp_init : _hal_rng_callback
- rng_ready_data_callback : _hal_rng_callback
- rng_state : rng_env_t
- role : app_i2c_params_t , i2c_env_t
- root_public_key_hash : __attribute__
- row_stride : app_graphics_dc_framelayer_t
- rpa_addr : ble_gap_evt_rslv_addr_report_t
- rr_intervals : hrs_c_hr_meas_t
- rr_intervals_num : hrs_c_hr_meas_t
- rsc_feature : rscs_c_evt_t
- rsc_meas_buff : rscs_c_evt_t
- rsc_sensor_loc : rscs_c_evt_t
- rscs_ctrl_pt_cccd_handle : rscs_c_handles_t
- rscs_ctrl_pt_handle : rscs_c_handles_t
- rscs_rsc_feature_handle : rscs_c_handles_t
- rscs_rsc_meas_cccd_handle : rscs_c_handles_t
- rscs_rsc_meas_handle : rscs_c_handles_t
- rscs_sensor_loc_handle : rscs_c_handles_t
- rscs_srvc_end_handle : rscs_c_handles_t
- rscs_srvc_start_handle : rscs_c_handles_t
- rslv_addr : ble_gapm_evt_t
- rslv_addr_report : ble_gapm_evt_t
- rsp : cgms_racp_rsp_t , gls_racp_rsp_t
- rsp_code_val : ras_ctr_pt_rsp_t
- rsp_data : ras_c_read_rsp_t
- rsp_id : hrrcps_rsp_val_t
- rsp_param : hrrcps_rsp_val_t
- rssi : ble_gap_conn_info_t , ble_gap_conn_iq_report_t , ble_gap_connless_iq_report_t , ble_gap_evt_adv_report_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_connless_iq_report_t , ble_gap_ext_adv_report_ind_t , thscps_test_info_t
- rssi_antenna_id : ble_gap_conn_iq_report_t , ble_gap_connless_iq_report_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_connless_iq_report_t
- rssi_cali : _efuse_trim0_t , rf_trim_info_t
- rsvd : ble_gap_ext_scan_param_t , ble_gap_per_sync_param_t
- rtc_alarm_callback : _hal_rtc_callback
- rtc_overflow_callback : _hal_rtc_callback
- rtc_tick_callback : _hal_rtc_callback
- rts : app_uart_pin_cfg_t
- run_addr : dfu_boot_info_t
- run_time : cgms_get_info_req_t
- rw_mode : _ll_qspi_memorymapped_init_t
- rx : app_uart_pin_cfg_t
- rx_abort_flag : uart_env_t
- rx_dma_channel : app_i2c_dma_cfg_t , app_i2s_dma_cfg_t , app_spi_dma_cfg_t , app_uart_dma_cfg_t
- rx_dma_instance : app_i2c_dma_cfg_t , app_i2s_dma_cfg_t , app_spi_dma_cfg_t , app_uart_dma_cfg_t
- rx_done : spi_env_t
- rx_handler_cb : gdx_lcp_config_t
- rx_hold_time : _i2c_init
- rx_path_comp : ble_gap_dev_rf_path_comp_ind_t
- rx_phy : ble_gap_conn_iq_report_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_phy_update_t , ble_gap_le_phy_ind_t , thscps_test_conn_info_t
- rx_sample_delay : _ll_qspi_init_t , _ll_qspi_memorymapped_init_t , _ll_spim_init_t , _qspi_init_t , _spi_init
- rx_state : _iso7816_handle_t , _uart_handle
- rx_threshold : _ll_i2s_init_t
- rx_timeout_mode : _uart_init
- rx_xfer_count : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- rx_xfer_size : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- rxdata_size : _ll_i2s_init_t