Macros
: data frame size in xip, take effect when enable DFS_HC
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_DATASIZE_8BIT
#define | LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_DATASIZE_16BIT
#define | LL_QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_DATASIZE_32BIT

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_BYTE

#define LL_QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_DATASIZE_8BIT

Definition at line 578 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD

#define LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_DATASIZE_16BIT

Definition at line 579 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_WORD

#define LL_QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_DATASIZE_32BIT

Definition at line 580 of file gr55xx_ll_qspi.h.