Macros
Mode
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Exported Constants

## Macros
#define | LL_GPIO_MODE_NONE ((uint32_t)0x0U)
#define | LL_GPIO_MODE_INPUT ((uint32_t)0x1U)
#define | LL_GPIO_MODE_OUTPUT ((uint32_t)0x2U)
#define | LL_GPIO_MODE_INOUT ((uint32_t)0x3U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_MODE_INOUT

#define LL_GPIO_MODE_INOUT ((uint32_t)0x3U)

Select input and output mode

Definition at line 172 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_MODE_INPUT

#define LL_GPIO_MODE_INPUT ((uint32_t)0x1U)

Select input mode

Definition at line 170 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_MODE_NONE

#define LL_GPIO_MODE_NONE ((uint32_t)0x0U)

No input or output

Definition at line 169 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_MODE_OUTPUT

#define LL_GPIO_MODE_OUTPUT ((uint32_t)0x2U)

Select output mode

Definition at line 171 of file gr55xx_ll_gpio.h.