Macros
frame format for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants

## Macros
#define | QSPI_CONCURRENT_XIP_FRF_RSVD LL_QSPI_CONCURRENT_XIP_FRF_RSVD
#define | QSPI_CONCURRENT_XIP_FRF_DUAL_SPI LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI
#define | QSPI_CONCURRENT_XIP_FRF_QUAD_SPI LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI
#define | QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_FRF_DUAL_SPI

#define QSPI_CONCURRENT_XIP_FRF_DUAL_SPI LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI

SPI Frame format : DUAL.

Definition at line 625 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI

#define QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI

SPI Frame format : OCTAL.

Definition at line 627 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_FRF_QUAD_SPI

#define QSPI_CONCURRENT_XIP_FRF_QUAD_SPI LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI

SPI Frame format : QUAD.

Definition at line 626 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_FRF_RSVD

#define QSPI_CONCURRENT_XIP_FRF_RSVD LL_QSPI_CONCURRENT_XIP_FRF_RSVD

SPI Frame format : Reserved.

Definition at line 624 of file gr55xx_hal_qspi.h.