Macros
: frame format for concurrent xip mode
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_FRF_RSVD 0x0
#define | LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI 0x1
#define | LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI 0x2
#define | LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI 0x3

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI 0x1

SPI Frame format : DUAL

Definition at line 634 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI 0x3

SPI Frame format : OCTAL

Definition at line 636 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI 0x2

SPI Frame format : QUAD

Definition at line 635 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_RSVD

#define LL_QSPI_CONCURRENT_XIP_FRF_RSVD 0x0

SPI Frame format : Reserved

Definition at line 633 of file gr55xx_ll_qspi.h.