### - r -

- RAS_AD_EVT_INVALID : ras_ad.h
- RAS_AD_EVT_SEND_NTI_IND_CMP : ras_ad.h
- RAS_AD_EVT_SET_CP_CCCD : ras_ad.h
- RAS_AD_EVT_SET_DATA_OW_CCCD : ras_ad.h
- RAS_AD_EVT_SET_DATA_READY_CCCD : ras_ad.h
- RAS_AD_EVT_SET_OD_DATA_CCCD : ras_ad.h
- RAS_AD_EVT_SET_RT_DATA_CCCD : ras_ad.h
- RAS_AD_EVT_WRITE_CP : ras_ad.h
- RAS_AD_IDX_CP_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_CP_CHAR : ras_ad.h
- RAS_AD_IDX_CP_VAL : ras_ad.h
- RAS_AD_IDX_DATA_OW_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_DATA_OW_CHAR : ras_ad.h
- RAS_AD_IDX_DATA_OW_VAL : ras_ad.h
- RAS_AD_IDX_DATA_READY_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_DATA_READY_CHAR : ras_ad.h
- RAS_AD_IDX_DATA_READY_VAL : ras_ad.h
- RAS_AD_IDX_FEA_CHAR : ras_ad.h
- RAS_AD_IDX_FEA_VAL : ras_ad.h
- RAS_AD_IDX_NB : ras_ad.h
- RAS_AD_IDX_OD_DATA_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_OD_DATA_CHAR : ras_ad.h
- RAS_AD_IDX_OD_DATA_VAL : ras_ad.h
- RAS_AD_IDX_RT_DATA_CCCD_CFG : ras_ad.h
- RAS_AD_IDX_RT_DATA_CHAR : ras_ad.h
- RAS_AD_IDX_RT_DATA_VAL : ras_ad.h
- RAS_AD_IDX_SVC : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_INDICATE : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_INVALID : ras_ad.h
- RAS_AD_SEND_DATA_TYPE_NOTIFY : ras_ad.h
- RAS_C_AD_CHAR_HANDLE_CCCD_NB : ras_c_ad.h
- RAS_C_AD_EVT_DISCOVER_COMPLETED : ras_c_ad.h
- RAS_C_AD_EVT_DISCOVER_FAILED : ras_c_ad.h
- RAS_C_AD_EVT_INVALID : ras_c_ad.h
- RAS_C_AD_EVT_READ_RSP : ras_c_ad.h
- RAS_C_AD_EVT_SERVER_IND : ras_c_ad.h
- RAS_C_AD_EVT_SERVER_NOTIFY : ras_c_ad.h
- RAS_C_AD_EVT_WRITE_ERR : ras_c_ad.h
- RAS_C_AD_EVT_WRITE_RSP : ras_c_ad.h
- RAS_C_AD_HANDLE_ON_DEMAND_RA_DATA : ras_c_ad.h
- RAS_C_AD_HANDLE_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_OVERWRITE : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_READY : ras_c_ad.h
- RAS_C_AD_HANDLE_RA_DATA_READY_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_CP : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_CP_IND_NTF_CFG : ras_c_ad.h
- RAS_C_AD_HANDLE_RAS_FEATURES : ras_c_ad.h
- RAS_C_AD_HANDLE_RT_RA_DATA : ras_c_ad.h
- RAS_C_AD_HANDLE_RT_RA_DATA_IND_NTF_CFG : ras_c_ad.h
- RAS_C_DIS_NTF_IND : ras_c.h
- RAS_C_EN_IND : ras_c.h
- RAS_C_EN_NTF : ras_c.h
- RAS_C_EN_NTF_IND : ras_c.h
- RAS_C_EVT_DISCOVER_COMPLETED : ras_c.h
- RAS_C_EVT_DISCOVER_FAILED : ras_c.h
- RAS_C_EVT_INVALID : ras_c.h
- RAS_C_EVT_READ_RSP : ras_c.h
- RAS_C_EVT_SUBEVT_REPORT : ras_c.h
- RAS_C_EVT_WRITE_ERR : ras_c.h
- RAS_C_EVT_WRITE_RSP : ras_c.h
- RAS_C_READ_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RA_DATA_READY_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RAS_CP_IND_NTF_CFG : ras_c.h
- RAS_C_READ_RAS_FEATURE : ras_c.h
- RAS_C_READ_RT_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_READ_TYPE_INVALID : ras_c.h
- RAS_C_WRITE_ON_DEMAND_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RA_DATA_OVERWRITE_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RA_DATA_READY_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RAS_CP : ras_c.h
- RAS_C_WRITE_RAS_CP_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_RT_RA_DATA_IND_NTF_CFG : ras_c.h
- RAS_C_WRITE_TYPE_INVALID : ras_c.h
- RAS_FEA_ABORT_OPERATION_BIT_MASK : ras_common.h
- RAS_FEA_ALL_BIT_MASK : ras_common.h
- RAS_FEA_FILTER_RA_DATA_BIT_MASK : ras_common.h
- RAS_FEA_RETR_LOST_RA_DATA_SEG_BIT_MASK : ras_common.h
- RAS_FEA_RT_RA_DATA_BIT_MASK : ras_common.h
- RAS_MODE_0 : ras_common.h
- RAS_MODE_1 : ras_common.h
- RAS_MODE_2 : ras_common.h
- RAS_MODE_3 : ras_common.h
- RAS_MODE_NUM : ras_common.h
- RAS_OP_ABORT_OPERATION : ras_common.h
- RAS_OP_ACK_RA_DATA : ras_common.h
- RAS_OP_CMP_LOST_RA_DATA_SEG_RSP : ras_common.h
- RAS_OP_CMP_RA_DATA_RSP : ras_common.h
- RAS_OP_FILTER : ras_common.h
- RAS_OP_GET_RA_DATA : ras_common.h
- RAS_OP_RETR_LOST_RA_DATA_SEGMENTS : ras_common.h
- RAS_OP_RSP_CODE : ras_common.h
- RAS_RSP_ABORT_UNSUCCESSFUL : ras_common.h
- RAS_RSP_INVALID_PARAM : ras_common.h
- RAS_RSP_NO_RECORDS_FOUND : ras_common.h
- RAS_RSP_OPCODE_NOT_SUPPORTED : ras_common.h
- RAS_RSP_PARAM_NOT_SUPPORTED : ras_common.h
- RAS_RSP_PROCEDURE_NOT_COMPLETED : ras_common.h
- RAS_RSP_SERVER_BUSY : ras_common.h
- RAS_RSP_SUCCESS : ras_common.h
- RNG_OSC_CLK : platform_sdk.h
- RNG_OSC_CLK2 : platform_sdk.h
- RNG_PWR_ID : app_pwr_mgmt.h
- RSCS_C_CTRL_PT_OP_REQ_SUP_LOC : rscs_c.h
- RSCS_C_CTRL_PT_OP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_OP_RSP_CODE : rscs_c.h
- RSCS_C_CTRL_PT_OP_SET_CUMUL_VAL : rscs_c.h
- RSCS_C_CTRL_PT_OP_START_CALIB : rscs_c.h
- RSCS_C_CTRL_PT_OP_UPD_LOC : rscs_c.h
- RSCS_C_CTRL_PT_RSP_FAILED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_INVALID_PARAM : rscs_c.h
- RSCS_C_CTRL_PT_RSP_NOT_SUP : rscs_c.h
- RSCS_C_CTRL_PT_RSP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_IND_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_RSP_RECEIVE : rscs_c.h
- RSCS_C_EVT_CTRL_PT_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_DISCOVERY_COMPLETE : rscs_c.h
- RSCS_C_EVT_DISCOVERY_FAIL : rscs_c.h
- RSCS_C_EVT_INVALID : rscs_c.h
- RSCS_C_EVT_RSC_FEATURE_RECEIVE : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_NTF_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_VAL_RECEIVE : rscs_c.h
- RSCS_C_EVT_SENSOR_LOC_RECEIVE : rscs_c.h
- RSCS_C_EVT_WRITE_OP_ERR : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_HUB : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_WHEEL : rscs_c.h
- RSCS_C_SENSOR_LOC_HIP : rscs_c.h
- RSCS_C_SENSOR_LOC_LEFT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_OTHER : rscs_c.h
- RSCS_C_SENSOR_LOC_RIGHT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_IN : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_TOP : rscs_c.h
- RSCS_C_SENSOR_LOC_SUP_NB : rscs_c.h
- RSCS_CTRL_PT_OP_REQ_SUP_LOC : rscs.h
- RSCS_CTRL_PT_OP_RESERVED : rscs.h
- RSCS_CTRL_PT_OP_RSP_CODE : rscs.h
- RSCS_CTRL_PT_OP_SET_CUMUL_VAL : rscs.h
- RSCS_CTRL_PT_OP_START_CALIB : rscs.h
- RSCS_CTRL_PT_OP_UPD_LOC : rscs.h
- RSCS_CTRL_PT_RSP_FAILED : rscs.h
- RSCS_CTRL_PT_RSP_INVALID_PARAM : rscs.h
- RSCS_CTRL_PT_RSP_NOT_SUP : rscs.h
- RSCS_CTRL_PT_RSP_RESERVED : rscs.h
- RSCS_CTRL_PT_RSP_SUCCESS : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_DISABLE : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_ENABLE : rscs.h
- RSCS_EVT_CTRL_POINT_RSP_CPLT : rscs.h
- RSCS_EVT_CUMUL_VAL_SET : rscs.h
- RSCS_EVT_INVALID : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_DISABLE : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_ENABLE : rscs.h
- RSCS_EVT_RSC_MEAS_SEND_CPLT : rscs.h
- RSCS_EVT_SEBSOR_CALIBRATION : rscs.h
- RSCS_EVT_SEBSOR_LOC_UPD : rscs.h
- RSCS_EVT_SUP_SEBSOR_LOC_REQ : rscs.h
- RSCS_SENSOR_LOC_FRONT_HUB : rscs.h
- RSCS_SENSOR_LOC_FRONT_WHEEL : rscs.h
- RSCS_SENSOR_LOC_HIP : rscs.h
- RSCS_SENSOR_LOC_LEFT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_OTHER : rscs.h
- RSCS_SENSOR_LOC_RIGHT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_SHOE_IN : rscs.h
- RSCS_SENSOR_LOC_SHOE_TOP : rscs.h
- RSCS_SENSOR_LOC_SUP_NB : rscs.h
- RTC_OSC_CLK : platform_sdk.h
- RTUS_CTRL_PT_CANCEL_UPDATE : rtus.h
- RTUS_CTRL_PT_GET_UPDATE : rtus.h
- RTUS_CUR_STATE_IDLE : rtus.h
- RTUS_CUR_STATE_PENDING : rtus.h
- RTUS_EVT_CANCEL_UPDATE : rtus.h
- RTUS_EVT_GET_UPDATE : rtus.h
- RTUS_EVT_INVALID : rtus.h
- RTUS_UPDATE_RESULT_CANCELED : rtus.h
- RTUS_UPDATE_RESULT_NO_ATTEMPTED : rtus.h
- RTUS_UPDATE_RESULT_NO_CONN_TO_REF : rtus.h
- RTUS_UPDATE_RESULT_REP_ERROR : rtus.h
- RTUS_UPDATE_RESULT_SCCESSFUL : rtus.h
- RTUS_UPDATE_RESULT_TIMEOUT : rtus.h