Macros
SPI Frame Format
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_FRF_SPI 0x00000000UL
#define | LL_QSPI_FRF_DUALSPI (1UL << QSPI_CTRL0_SPIFRF_Pos)
#define | LL_QSPI_FRF_QUADSPI (2UL << QSPI_CTRL0_SPIFRF_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_FRF_DUALSPI

#define LL_QSPI_FRF_DUALSPI (1UL << QSPI_CTRL0_SPIFRF_Pos)

Dual-SPI frame format for transfer

Definition at line 381 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_FRF_QUADSPI

#define LL_QSPI_FRF_QUADSPI (2UL << QSPI_CTRL0_SPIFRF_Pos)

Quad-SPI frame format for transfer

Definition at line 382 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_FRF_SPI

#define LL_QSPI_FRF_SPI 0x00000000UL

SPI frame format for transfer

Definition at line 380 of file gr55xx_ll_qspi.h.