Public Attributes | List of all members
_ll_xqspi_hp_init_t Struct Reference
Peripheral Driver » LL Driver » XQSPI » Structures » XQSPI Exported init structure

XQSPI High Performance mode init structures definition. More...

`#include <gr55xx_ll_xqspi.h>`

## Public Attributes
uint8_t | xqspi_hp_enable
uint8_t | xqspi_hp_cmd
uint8_t | xqspi_hp_end_dummy

## Detailed Description

XQSPI High Performance mode init structures definition.

Definition at line 76 of file gr55xx_ll_xqspi.h.

## Member Data Documentation

## ◆ xqspi_hp_cmd

uint8_t _ll_xqspi_hp_init_t::xqspi_hp_cmd

Specifies the command to enter HP mode for XQSPI.

Definition at line 81 of file gr55xx_ll_xqspi.h.

## ◆ xqspi_hp_enable

uint8_t _ll_xqspi_hp_init_t::xqspi_hp_enable

Specifies If enable the HP mode for XQSPI. This parameter can be a value of XQSPI HP mode

Definition at line 78 of file gr55xx_ll_xqspi.h.

## ◆ xqspi_hp_end_dummy

uint8_t _ll_xqspi_hp_init_t::xqspi_hp_end_dummy

Specifies the end dummpy cycle in HP mode for XQSPI.

Definition at line 83 of file gr55xx_ll_xqspi.h.

The documentation for this struct was generated from the following file:

- gr55xx_ll_xqspi.h