Enumerations
HAL RNG state
Peripheral Driver » HAL Driver » RNG » Enumerations

## Enumerations
enum | hal_rng_state_t { HAL_RNG_STATE_RESET = 0x00, HAL_RNG_STATE_READY = 0x01, HAL_RNG_STATE_BUSY = 0x02, HAL_RNG_STATE_TIMEOUT = 0x03, HAL_RNG_STATE_ERROR = 0x04 }
| HAL RNG State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_rng_state_t

enum hal_rng_state_t

HAL RNG State Enumerations definition.

Enumerator
HAL_RNG_STATE_RESET | RNG not initialized or disabled yet
HAL_RNG_STATE_READY | RNG initialized and ready for use
HAL_RNG_STATE_BUSY | RNG internal process is ongoing
HAL_RNG_STATE_TIMEOUT | RNG timeout state
HAL_RNG_STATE_ERROR | RNG error state

Definition at line 75 of file gr55xx_hal_rng.h.