Macros
AON_GPIOEx Mux Mode definition
Peripheral Driver » HAL Driver » AON_GPIOEx » Defines » AON_GPIOEx Exported Constants

## Macros
#define | AON_GPIO_MUX_0 LL_AON_GPIO_MUX_0
#define | AON_GPIO_MUX_1 LL_AON_GPIO_MUX_1
#define | AON_GPIO_MUX_2 LL_AON_GPIO_MUX_2
#define | AON_GPIO_MUX_3 LL_AON_GPIO_MUX_3
#define | AON_GPIO_MUX_4 LL_AON_GPIO_MUX_4
#define | AON_GPIO_MUX_5 LL_AON_GPIO_MUX_5
#define | AON_GPIO_MUX_6 LL_AON_GPIO_MUX_6
#define | AON_GPIO_MUX_7 LL_AON_GPIO_MUX_7
#define | AON_GPIO_MUX_8 LL_AON_GPIO_MUX_8

## Detailed Description

## Macro Definition Documentation

## ◆ AON_GPIO_MUX_0

#define AON_GPIO_MUX_0 LL_AON_GPIO_MUX_0

AON GPIO Mux mode 0

Definition at line 78 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_1

#define AON_GPIO_MUX_1 LL_AON_GPIO_MUX_1

AON GPIO Mux mode 1

Definition at line 79 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_2

#define AON_GPIO_MUX_2 LL_AON_GPIO_MUX_2

AON GPIO Mux mode 2

Definition at line 80 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_3

#define AON_GPIO_MUX_3 LL_AON_GPIO_MUX_3

AON GPIO Mux mode 3

Definition at line 81 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_4

#define AON_GPIO_MUX_4 LL_AON_GPIO_MUX_4

AON GPIO Mux mode 4

Definition at line 82 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_5

#define AON_GPIO_MUX_5 LL_AON_GPIO_MUX_5

AON GPIO Mux mode 5

Definition at line 83 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_6

#define AON_GPIO_MUX_6 LL_AON_GPIO_MUX_6

AON GPIO Mux mode 6

Definition at line 84 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_7

#define AON_GPIO_MUX_7 LL_AON_GPIO_MUX_7

AON GPIO Mux mode 7

Definition at line 85 of file gr55xx_hal_aon_gpio_ex.h.

## ◆ AON_GPIO_MUX_8

#define AON_GPIO_MUX_8 LL_AON_GPIO_MUX_8

AON GPIO Mux mode 8

Definition at line 86 of file gr55xx_hal_aon_gpio_ex.h.