### - w -

- wait_cycles : _ll_qspi_init_t
- wait_time : _ll_iso7816_init , iso7816_init_t
- warning : __attribute__
- wdt_msp_deinit : _hal_wdt_callback
- wdt_msp_init : _hal_wdt_callback
- wdt_period_elapsed_callback : _hal_wdt_callback
- week : _calendar_time
- weight : bcs_meas_val_t , uds_chars_val_t , wss_meas_val_t
- weight_present : bcs_meas_flag_t , uds_chars_flag_t
- wfi_clk : _cgc_init
- wheel_rev_data_present : cscs_meas_val_t
- window : ble_gap_scan_param_t
- work_mode : _xqspi_init_t
- wr : _ll_qspi_memorymapped_init_t
- wr_lc : app_graphics_ospi_params_t
- write_fifo : _dspi_handle , _i2s_handle , _qspi_handle , _spi_handle
- write_req : ble_gatts_evt_t
- write_rsp : ble_gattc_evt_t , ras_c_ad_evt_t , ras_c_evt_t
- write_type : ras_c_write_req_t , ras_c_write_rsp_t
- ws : app_i2s_pin_cfg_t
- ws_cycles : _i2s_init , _ll_i2s_init_t
- wss_height_res : wss_init_t
- wss_mass_res : wss_init_t
- wss_unit : wss_init_t