Public Attributes | List of all members
bms_init_t Struct Reference
BLE Services » Bond Management Service (BMS) » Structures

BMS Service init stucture. This contains all option and data needed for initialization of the service. More...

`#include <bms.h>`

## Public Attributes
bms_cccd_change_handler_t | cccd_change_handler
uint32_t | feature
uint8_t | auth_code_val [BMS_AUTH_CODE_LEN_MAX]
uint8_t | auth_code_len

## Detailed Description

BMS Service init stucture. This contains all option and data needed for initialization of the service.

Definition at line 145 of file bms.h.

## Member Data Documentation

## ◆ auth_code_len

uint8_t bms_init_t::auth_code_len

Definition at line 151 of file bms.h.

## ◆ auth_code_val

uint8_t bms_init_t::auth_code_val[BMS_AUTH_CODE_LEN_MAX]

Definition at line 150 of file bms.h.

## ◆ cccd_change_handler

bms_cccd_change_handler_t bms_init_t::cccd_change_handler

Definition at line 148 of file bms.h.

## ◆ feature

uint32_t bms_init_t::feature

Definition at line 149 of file bms.h.

The documentation for this struct was generated from the following file:

- bms.h